{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[13,0,13,7]]}
[]
[null,"235TLA","250TLA","250TLA IV","260TLA","270TL"]
["Tractor Family/Series"]
["Tractor Compatibility ","Boomer™ 24","Boomer™ 33 & 37 ROPS and Boomer 37 Cab","Boomer™ 3040, 3045, 3050 CVT Cab | Boomer 45D & 50D | Boomer 46D & 54D","Boomer™ 41 & 47 ROPS and Cab","WORKMASTER™ 45 & 55"]
["Loader Specifications"]
["Max Lift Height to Bucket Pivot Pins (ft. (mm)) ","6.7 (2050)","8.6 (2642)","8.7 (2642)","9 (2769)","9.1 (2768)"]
["Dump Clearance (ft. (mm)) ","–","6.4 (1956)","6.4 (1956)","6.7 (2032)","-"]
["Digging Depth (in. (mm)) ","3.9 (100)","6.8 (173)","6.8 (173)","6.3 (160)","4.5 (114)"]
["Lift Capacity to 1500 mm @ Pivot Pins (lbs. (kg)) ","1034 (470)","2176 (987)","2176 (987)","2256 (1023)","3254 (1476)"]
["Breakout Force @ Pivot Pins (lbs. (kg)) ","1,672 (760)","3257 (1477)","3257 (1477)","4081 (1851)","4303 (1952)"]
["Reach at Max Height (in. (mm)) ","25.2 (640)","48 (1219)","48 (1219)","58 (1473)","-"]
["Maximum Bucket Rollback Angle (degrees) ","29","30","30","28","34"]
["Maximum Bucket Dump Angle (degrees) ","51","48","48","56","57"]
["     See product brochure for full specifications and options."]