{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":89,"n_cols":3,"rows_kept":89,"cut":false,"hidden":false,"merged":[[88,0,88,4]]}
[]
[null,"Braud 7030M","Braud 8030L"]
["Vineyard row spacing"]
["Vineyard row spacing (ft. (m)) ","Intermediate > 4.26 (> 1.3)","Large > 5.24 (> 1.6)"]
["Engine"]
["Type ","FPT NEF","FPT NEF"]
["Compliant with engine emissions regulations ","Tier 4B/Stage 4","Tier 4B/Stage 4"]
["Power ECE R120/ISO 14396 (hp (kW(CV))) ","128 (94)","128 (94)"]
["Cylinders / Aspiration / Displacement (in.³ (cm³)) ","4 / Turbo with Intercooler / 274 (4485)","4 / Turbo with Intercooler / 274 (4485)"]
["ECOBlue™ HI-eSCR system (Selective Catalytic Reduction) ","Standard","Standard"]
["Reversible cooling fan ","Standard","Standard"]
["Tractor base unit"]
["Diesel capacity / AdBlue® capacity (gal. (L)) ","42.3/10.8 (160/41)","42.3/10.8 (160/41)"]
["Heavy Duty Hydrostatic transmission with Anti-Skid system ","Standard","Standard"]
["Road speed (15.5 mph (25kph)) with reduced engine (rpm) ","Standard","Standard"]
["Maximum steering angle (degrees) ",90,90]
["Front wheel torque limiter ","Standard","Standard"]
["Maximum slope (with auger) (%) ",32,32]
["Maximum slope (with destemmer) (%) ",30,30]
["Maximum slope (with Opti-Grape™) (%) ",25,"–"]
["Maximum lateral slope (%) ",25,25]
["IMS 2.0 - Intelligent Management System 2.0 ","Standard","Standard"]
["CDHA - Automatic height and lateral slope correction ","Standard","Standard"]
["Cruise control with radar ","Standard","Standard"]
["Electric park brake with brake pedal and seat button ","Standard","Standard"]
["Front multifunction tool carrier ","Optional","Optional"]
["Harvesting head"]
["Number of SDC shakers (standard) ",12,14]
["Low grape shaker rods ","Standard","Standard"]
["Flexible rear shaker fixation ","Standard","Standard"]
["Semi-Quick coupling of the picking head ","Standard","Standard"]
["Electric Shaker rod aperture adjustment ","Standard","Standard"]
["Quick release shaker plate ","Standard","Standard"]
["Ground sensors ","Standard","Standard"]
["Sealed length of collection baskets (in. (mm)) ","74.8 (1900)","82.7 (2100)"]
["Number of collection baskets ","2x54","2x58"]
["Basket size ","STD 3 rivets","XXL 4 rivets"]
["Noria tensioning system ","Standard","Standard"]
["Easy head swing lock system ","Standard","Standard"]
["High capacity cleaning conveyors (in. (mm)) ","17.7 (450)","23.6 (600)"]
["Upper cleaning fans ","Standard","Standard"]
["Rear fan exhaust with flap ","Standard","Standard"]
["Stainless steel hoppers (gal. (L)) ","607.6 (2300)","660.4 / 739.7 (2500 / 2800)"]
["Destemmer with crop spreader and AutoFill ","Standard","Optional"]
["Opti-Grape™ with crop spreader and AutoFill ","Optional","–"]
["Harvesting head centralized greasing ","Standard","Standard"]
["Washing water supply pipe and valve ","Standard","Standard"]
["Washing external buttons ","Standard","Standard"]
["Magnets ","Standard","Standard"]
["Cab"]
["Cab inside volume (ft³ (m³)) ","76.6 (2.17)","78.8 (2.23)"]
["Cab glass area (ft³ (m³)) ","79.5 (2.25)","80.2 (2.27)"]
["Actuated access ladder and platform with light ","Standard","Standard"]
["Protective structure ","ROPS code 4","ROPS code 4"]
["Air conditioning and refrigerated box ","Standard","Standard"]
["Cab filtration system / Category level (EN 15695) ","Standard / 2","Standard / 2"]
["Bluetooth® Radio with separated microphone (hands free phone calls) ","Standard","Standard"]
["2 speakers integrated system ","Standard","Standard"]
["Adjustable armrest & multifunctional joystick ","Standard","Standard"]
["IntelliView™ IV touch screen monitor with adjustable position ","Standard","Standard"]
["Split screen color monitor for cameras ","Standard","Standard"]
["Cameras (color) ","2 Standard / +2 Optional","2 Standard / +2 Optional"]
["Steering column and adjustable seat ","Standard","Standard"]
["Lights with dedicated Light Control Panel (LCP) ",12,12]
["Mirrors with electrical adjustment ","Standard","Standard"]
["Right mirrors retractable ","Standard","Standard"]
["Front and rear sunshades ","Standard","Standard"]
["Blue Cab™ 4 system Pack"]
["Featuring Category 4 filtration (EN 15695-1 and -2) ","Standard","Optional"]
["Automatic A/C ","Standard","Optional"]
["Heated and ventilated two tone deluxe seat ","Standard","Optional"]
["LED working ","Standard","Optional"]
["Removable 12V Cool box (only for 8030L with Blue Cab™ 4 system) ","N/A","Optional"]
["Premium Viticulture/PLM"]
["Row Tracking system GPS NH 162 (RTS) ","Optional","Optional"]
["Hopper level indicator (progressive) ","Optional","Optional"]
["Dimensions and tires"]
["Front tires available ","320-70R20 / 340-80R18","340-80R18 / 400-70R18"]
["Rear tires available ","340-85R24","420-70R24 / 460-70R24"]
["Maximum height with cab, harvesting head on the ground (ft. in. (m)) ","11’ 11” (3.63)","11’ 10” (3.60)"]
["Maximum length (ft. in. (m)) ","16’ 6” (5.03)","17’ (5.17)"]
["Maximum width of base unit (ft. in. (m)) ","8’ 7” (2.61)","9’ 1” (2.77)"]
["Width with harvesting head fitted at the rear wheels (ft. in. (m)) ","7’ 1” (2.15)","8’ 10” (2.69)"]
["Ground clearance (ft. in. (m)) ","5’ 11” to 7’ 7” (1.80 to 2.30)","6’ 5” to 8’ (1.95 to 2.45)"]
["Wheelbase (ft. in. (m)) ","9’ 1” (2.78)","9’ 1” (2.78)"]
["Maximum hopper tipping height, under hopper (ft. in. (m)) ","7’ 11” (2.41)","8’ 3” (2.51)"]
["Maximum hopper tipping axis height (ft. in. (m)) ","8’ 4” (2.53)","8’ 8” (2.63)"]
["Harvesting head rear offset (from wheel axle) (ft. in. (m)) ","2’ 0” (0.62)","2’ 6” (0.76)"]
["&ndash; Not available "]