{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[[51,0,51,9]]}
[]
[null,"Durabine™ 413 PLUS","Durabine™ 416 PLUS","Durabine™ 419 PLUS","Durabine™ 416 PLUS Specialty","Haybine® 14HS","Haybine® 16HS","Haybine® 18HS"]
["Dimensions & Weights"]
["Cutting width (ft. in. (m)) ","13' 1\" (4.0)","16' 3\" (4.95)","19' 4\" (5.9)","16' 3\" (4.95)","14' 3\" (4.34)","16' 3\" (4.95)","18' 3\" (5.56)"]
["Overall width (ft. in. (m)) ","13' 6\" (4.11)","16' 7\" (5.05)","19' 5\" (5.91)","16' 7\" (5.05)","16' 3\" (4.95)","18' 3\" (5.56)","20' 3\" (6.17)"]
["Weighting with conditioning system (lbs. (kg)) ","3880 (1760)","5114 (2319)","5754 (2609)","–","3900 (1770)","4120 (1869)","4370 (1983)"]
["Weight less conditioning system (lbs. (kg)) ","-","-","-","5114 (2319)","-","-","-"]
["Durabine PLUS MowMax™ II PLUS Cutterbar"]
["Cutting width (ft. in. (m)) ","13' 1\" (4.0)","16' 3\" (4.95)","19' 4\" (5.9)","16' 3\" (4.95)","-","-","-"]
["Cutting height range (in. (mm)) ",".5 - 3.3 (13 - 86)",".5 - 3.3 (13 - 86)","0.5-3.3 (13 - 86)","0.5-3.3 (13 - 86)","-","-","-"]
["Cutting angle (degrees) ","-2 to -10 ","0 to -10"," 0 to -10"," 0 to -10","-","-","-"]
["Number of discs ",8,10,12,10,"-","-","-"]
["Maximum disc speed (rpm) ",2300,2600,2600,2600,"-","-","-"]
["Number of reversible, swing-away knives ",16,20,24,20,"-","-","-"]
["Knife tip speed (mph (kph)) ","171 (275)","195 (314)","195 (314)","195 (314)","-","-","-"]
["Flotation ","Hydraulic adjustment from cab","Hydraulic adjustment from cab","Hydraulic adjustment from cab","Hydraulic adjustment from cab","-","-","-"]
["ShockPRO™ Disc Drive Protection System ","Standard","Standard","Standard","Standard","-","-","-"]
["3-Year MowMax™ Factory Cutterbar Warranty ","Standard","Standard","Standard","Standard","-","-","-"]
["Haybine Cutterbar"]
["Cutting width (ft. in. (m)) ","-","-","–","–","14' 3\" (4.34)","16' 3\" (4.95)","18' 3\" (5.56)"]
["Cutting height range (in. (mm)) ","-","-","–","–","1.2-6.2 (30.5-157.5)","1.2-6.2 (30.5-157.5)","1.2-6.2 (30.5-157.5)"]
["Cutting angle (degrees) ","-","-","–","–","-6 to -12 ","-6 to -12","-6 to -12"]
["Type ","-","-","–","–","Timed, dual, counterstroking","Timed, dual, counterstroking","Timed, dual, counterstroking"]
["Knives ","-","-","–","–","Over serrated, bolted","Over serrated, bolted","Over serrated, bolted"]
["Guards ","-","-","–","–","2-tine, double-hardened","2-tine, double-hardened","2-tine, double-hardened"]
["Skid shoes ","-","-","–","–",4,4,4]
["Drive type ","-","-","–","–","Open, dual, wobble","Open, dual, wobble","Open, dual, wobble"]
["Speed (spm) ","-","-","–","–",1810,1810,1810]
["Stroke (in. (mm)) ","-","-","–","–","3 (76)","3 (76)","3 (76)"]
["Haybine Reel"]
["Type ","-","-","–","–","5 bat","5 bat","5 bat"]
["Adjustments ","-","-","–","–","Fore/aft and vertical","Fore/aft and vertical","Fore/aft and vertical"]
["Mechanical drive (rpm) ","-","-","–","–","58 - 83","58 - 83","58 - 83"]
["Hydraulic drive (optional) (rpm) ","-","-","–","–","0 - 76","0 - 76","0 - 76"]
["Speed adjustment (mechanical) ","-","-","–","–","Variable sheave","Variable sheave","Variable sheave"]
["Diameter (in. (mm)) ","-","-","–","–","42 (1067)","42 (1067)","42 (1067)"]
["Drive type ","-","-","–","–","Belt and chain","Belt and chain","Belt and chain"]
["Tine bars ","-","-","–","–","Segmented","Segmented","Segmented"]
["Bushings / bearings* (in. (mm)) ","-","-","–","–","1.25 (31.75)","1.25 (31.75)","1.25 (31.75)"]
["Auger"]
["Auger diameter (in. (mm)) ","-","20 (508)","20 (508)","20 (508)","20 (508)","20 (508)","20 (508)"]
["Auger type ","-","Floating","Floating","Floating, gentle-flow tapered","Floating","Floating","Floating"]
["Conditioning Systems"]
["Roll types ","Chevron pattern rubber or steel","Chevron pattern rubber or steel or B&D's \"The Crusher\" rubber rolls","Chevron pattern rubber or steel or B&D's \"The Crusher\" rubber rolls","-","Chevron pattern rubber or steel","Chevron pattern rubber or steel","Chevron pattern rubber or steel"]
["Roll length (in. (mm)) ","125 (3175)","102 (2591)","102 (2591)","-","102 (2591)","102 (2591)","102 (2591)"]
["Roll diameter (in. (mm)) ","10.4 (263)","10.16 (258)","10.16 (258)","-","10 .16 (258)","10 .16 (258)","10 .16 (258)"]
["Roll speed (rpm) ","750 (or 640 swapping roll sheaves)",938,938,"-",717,717,717]
["Roll pressure ","Hand crank","Hand crank","Hand crank","-","Hand crank","Hand crank","Hand crank"]
["Roll gap ","Adjustable stop-bolt","Adjustable stop-bolt","Adjustable stop-bolt","-","Adjustable stop-bolt","Adjustable stop-bolt","Adjustable stop-bolt"]
["Roll drive ","Spur gearbox and PTO","Spur gearbox and PTOs","Spur gearbox and PTOs","-","Spur gearbox and PTOs","Spur gearbox and PTOs","Spur gearbox and PTOs"]
["Windrow/swath width (in. (mm)) ","38 to 96 (965 to 2438)","38 to 96 (965 to 2438)","38 to 96 (965 to 2438)","60 or 83 (1524 to 2108) Swath Closure Kit","38 to 96 (965 to 2438)","38 to 96 (965 to 2438)","38 to 96 (965 to 2438)"]
["    * Bearing with collar at cam end. Bushings at all other locations. "]