{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":68,"n_cols":11,"rows_kept":68,"cut":false,"hidden":false,"merged":[[67,0,67,12]]}
[]
[null,"P2080 - 30 ft","P2080 - 40 ft","P2080 - 50 ft","P2080 - 60 ft","P2082 – 30 ft","P2082 – 40 ft","P2082 – 50 ft","P2082 – 60 ft","P2185 - 30 ft","P2185 - 40 ft"]
["Specifications"]
["Toolbar Width (ft. (m)) ","30 (9.1)","40 (12.2)","50 (15.2)","60 (18.3)","30 (9.1)","40 (12.2)","50 (15.2)","60 (18.3)","30 ft. (9.1)","40 ft. (12.2)"]
["Available Spacing (in. (cm)) ","7.5 (19.1) & 10 (25.4)","7.5 (19.1) & 10 (25.4)","7.5 (19.1) & 10 (25.4)","7.5 (19.1) & 10 (25.4)","10 (25.4)","10 (25.4)","10 (25.4)","10 (25.4)","7.5 (19.1) & 10 (25.4) &15 (38.1)","7.5 (19.1) & 10 (25.4) &15 (38.1)"]
["Transport height (ft. (m)) ","13 (3.96)","13.8 (4.2)","13.2 (4.0)","14.75 (4.5)","13.1 (3.99)","13.7 (4.17)","13.2 (4.02)","14.8 (4.5)","13' 1\" (3.99)","13' 10\" (4.23)"]
["Transport width (ft. (m)) ","12 (3.65)","18.5 (5.63)","18.7 (5.7)","18.7 (5.7)","12 (3.66)*","18.7 (5.69)*","18.7 (5.69)*","18.7 (5.69)*","12 (3.65)","18.5 (5.63)"]
["Road-to-Opener Clearance (in. (cm)) ","8.5 (21.6)","8.5 (21.6)","8.5 (21.6)","8.5 (21.6)","8.5 (21.6)","8.5 (21.6)","8.5 (21.6)","8.5 (21.6)","8' 6\" (21.6)","8' 6\" (21.6)"]
["Weight - 7.5 in. (19.1 cm) - spacing (empty) (lbs. (kg)) ","19,600 (8900)","24,800 (11,250)","40000 (18144)","45500 (20412)","–","_","–","–","22,890 (10,380)","28,360 (12,860)"]
["Weight 10 in. (25.4 cm) - spacing (empty) (lbs. (kg)) ","17,500 (7900)","22,100 (10,000)","36000 (16329)","41500 (18597)","21,200 (9615)","27,800 (12,610)","41,500 (18,825)","43,500 (19,730)","20,890 (9475)","25,660 (11,640)"]
["Weight 15 in. (38.1 cm) - spacing (empty) (lbs. (kg)) ","_","_","_","_","_","_","_","_","17,790 (8070)","22,380 (10,150)"]
["Length with rear hitch (pin to pin) (ft. (m)) ","36.4  (11.09 )","38.6 (11.76)","38.6 (11.76)","38.6 (11.76)","36.4 (11.09)","38.6 (11.76)","38.6 (11.76)","38.6 (11.76)","_","_"]
["Split rank capability (in. (cm)) ","15 (38.1) 20 (50.8)","15 (38.1) 20 (50.8)","15 (38.1)","15 (38.1)","20 (50.8)","20 (50.8)","20 (50.8)","20 (50.8)","15 (38.1) 20 (50.8)","15 (38.1) 20 (50.8)"]
["Number of row units - 7.5 in. (19.1 cm) spacing ",48,64,80,96,"–","–","–","–",48,64]
["Number of row units - 10 in. (25.4 cm) spacing ",36,48,60,72,36,48,60,72,36,48]
["Number of row units -  15 in. (38.1 cm) spacing ","_","_","_","_","_","_","_","_",24,32]
["Minimum tractor PTO hp required - 7.5 in. (19.1 cm) spacing* ",195,260,304,364.8,"–","–","–","–",195,260]
["Minimum tractor PTO hp required 10 in. (25.4 cm) spacing* ",145,195,228,273.6,216,288,360,432,145,195]
["Minimum tractor PTO hp required 15 in. (38.1 cm) spacing* ","_","_","_","_","_","_","_","_",98,131]
["Minimum tractor PTO hp required 7.5 in. (19.1 cm) spacing with air cart* ","260 to 295","325 to 360","369 to 404","430 to 465","–","–","–","–","260 to 295","325 to 360"]
["Minimum tractor PTO hp required 10 in. (25.4 cm) spacing with air cart* ","210 to 245","260 to 295","293 to 328","339 to 374","–","–","–","–","210 to 245","_"]
["Fold Type ","Single","Single","Double","Double","Single","Single","Double","Double","Single","Single"]
["Wing Sections ",3,3,5,5,3,3,5,5,3,3]
["Tires total ","12 (16 optional)","12 (16 optional)","20 (24 optional)","20 (24 optional)","12 (16 optional)","12 (16 optional)","20 (24 optional)","20 (24 optional)",16,16]
["Center section walking beam castor tires ","12.5L x15","12.5L x15","16.5 x 16.1 E","16.5 x 16.1 E","12.5L x 15","12.5L x 15","16.5 x 16.1 E","16.5 x 16.1 E","380 / 55 R 16.5 D ply","380 / 55 R 16.5 D ply"]
["Rear mainframe dual walking beam tire size ","18L x 16.1","18L x 16.1","16.5 x 16.1 E","16.5 x 16.1 E","18L x 16.1","18L x 16.1","16.5 x 16.1 E","16.5 x 16.1 E","380 / 55 R 16.5 E ply","380 / 55 R 16.5 E ply"]
["High Flotation Rear Mainframe dual walking beam tire size ","_","_","_","_","_","_","_","_","500 / 40 R 16.5 E ply","500 / 40 R 16.5 E ply"]
["Inner and outer wings walking beam castor tire size ","12.5L x15","12.5L x15","12.5L x15","12.5L x15","12.5L x 15","12.5L x 15","12.5L x 15","12.5L x 15","340 / 60 R 15 D ply","340 / 60 R 15 D ply"]
["Operating Speed (mph (kph)) ","5-8 (8-12.7)","5-8 (8-12.7)","5-8 (8-12.7)","5-8 (8-12.7)","4.5 to 8 (7.2-12.9)","4.5 to 8 (7.2-12.9)","4.5 to 8 (7.2-12.9)","4.5 to 8 (7.2-12.9)","5-8 (8-12.7)","5-8 (8-12.7)"]
["Hitch Type ","Floating","Floating","Floating","Floating","Floating","Floating","Floating","Floating","Floating","Floating"]
["Ground following design ","Parallel link","Parallel link","Parallel link","Parallel link","Parallel link","Parallel link","Parallel link","Parallel link","Parallel link","Parallel link"]
["Row unit travel from level surface (in. (cm)) ","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down","8.5 (21.6) up, 11.5 (29.2) down"]
["Wing flex ","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down","15 degrees up, 10 degrees down"]
["Discs (in. (cm)) ","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees","18 (45.7) at 7 degrees"]
["Gauge wheel options ","_","_","_","_","_","_","_","_","3\" x 16\" or 4.5\" x 16\" solid or spoked","3\" x 16\" or 4.5\" x 16\" solid or spoked"]
["Depth settings (in. (cm)) ","14 position T-handle adjust from 0 to 3.5 (8.9)","14 position T-handle adjust from 0 to 3.5 (8.9)","14 position T-handle adjust from 0 to 3.5 (8.9)","14 position T-handle adjust from 0 to 3.5 (8.9)","17 position/notches T-handle adjust from 1/2 to 2” (1.3 to 5.1)","17 position/notches T-handle adjust from 1/2 to 2” (1.3 to 5.1)","7 position/notches T-handle adjust from 1/2 to 2” (1.3 to 5.1)","17 position/notches T-handle adjust from 1/2 to 2” (1.3 to 5.1)","14 position T-handle adjust from 0 to 3.5 (8.9)","14 position T-handle adjust from 0 to 3.5 (8.9)"]
["Down pressure adjustment ","Variable spring","Variable spring","Variable spring","Variable spring","In cab adjustable hydraulic","In cab adjustable hydraulic","In cab adjustable hydraulic","In cab adjustable hydraulic","Variable spring","Variable spring"]
["Closing wheel variable packing pressure (lbs. (kg)) ","60, 75 or 85 (27.2, 34 or 38.6)","60, 75 or 85 (27.2, 34 or 38.6)","60, 75 or 85 (27.2, 34 or 38.6)","60, 75 or 85 (27.2, 34 or 38.6)","59, 71 or 84 (26.8, 32.2 or 38.1)","59, 71 or 84 (26.8, 32.2 or 38.1)","59, 71 or 84 (26.8, 32.2 or 38.1)","59, 71 or 84 (26.8, 32.2 or 38.1)","60, 70 or 85 (27.2, 31.8 or 38.6)","60, 70 or 85 (27.2, 31.8 or 38.6)"]
["Standard in-cab down pressure control (lbs. (kg)) ","200 to 1400 (91 to 635)","200 to 1400 (91 to 635)","200 to 1400 (91 to 635)","200 to 1400 (91 to 635)","200 to 1300 (91 to 590)","200 to 1450 psi (91 to 658)","200 to 1450 psi (91 to 658)","200 to 1450 psi (91 to 658)","200 to 1400 (91 to 635)","200 to 1400 (91 to 635)"]
["Hydraulic requirements (gpm (Lpm)) ","30 (114) – 3 remotes","30 (114) – 3 remotes","30 (114) – 3 remotes","30 (114) – 3 remotes","15 (57) – 2 remotes","15 (57) – 2 remotes","30 (114) – 2 remotes","30 (114) – 2 remotes","30 (114) – 3 remotes","30 (114) – 3 remotes"]
["Hydraulic system ","In cab down pressure adjust standard","In cab down pressure adjust standard","In cab down pressure adjust standard","In cab down pressure adjust standard","–","–","–","–","In cab down pressure adjust standard","In cab down pressure adjust standard"]
["Tow between/behind air cart capacity (bu. (L)) ","280 to 430 (9867 to 15153)","280 to 430 (9867 to 15153)","280 to 580 (9867 to 20439)","280 to 580 (9867 to 20439)","–","–","–","–","_","_"]
["Mounted Seed tank capacity (bu. (L)) ","_","_","_","_","–","–","–","–","110 (3876)","140 (4933)"]
["Mounted tank ","_","_","_","_","–","–","–","–","_","_"]
["Display system ","Intelliview IV or ISO11783 compliant display","Intelliview IV or ISO11783 compliant display","Intelliview IV or ISO11783 compliant display","Intelliview IV or ISO11783 compliant display","–","–","–","–","Requires an ISO11783 compliant display such as Intelliview IVTM","Requires an ISO11783 compliant display such as Intelliview IV™"]
["Sectional control ","1/2 width  - optional DIA on Air Cart","1/2 width  - optional DIA on Air Cart","1/2 width  - optional DIA on Air Cart","1/2 width  - optional DIA on Air Cart","–","–","–","–","4-section metering with overlap control","4-section metering with overlap control"]
["Blockage Monitoring ","Optional","Optional","Optional","Optional","Optional IntelligentAg© Recon Wireless Blockage and Flow Monitor","Optional IntelligentAg© Recon Wireless Blockage and Flow Monitor","Optional IntelligentAg© Recon Wireless Blockage and Flow Monitor","Optional IntelligentAg© Recon Wireless Blockage and Flow Monitor","Outback blockage","Outback blockage"]
["Optional equipment"]
["High flotation tire option ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Hydraulic work switch ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Weight bracket ","Optional","Optional","Optional","Optional","–","–","–","–","Optional","Optional"]
["Meter roll selection (extra fine, fine, coarse) ","Optional","Optional","Optional","Optional","–","–","–","–","Optional","Optional"]
["Auxiliary rear hitch ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","–","–"]
["4-section metering with overlap control ","–","–","–","–","–","–","–","–","Optional","Optional"]
["Cross tillage hydraulic package ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","–","–"]
["GPS speed sensor ","–","–","–","–","–","–","–","–","Optional","Optional"]
["Split-rank header insert, 7.5 in. (19.1 cm) ","Optional","Optional","Optional","Optional","–","–","–","–","–","–"]
["Primary run blockage ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","–","–"]
["Secondary run (all run) blockage hydraulic work switch ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","–","–"]
["1/2 width sectional control on air cart ","Optional","Optional","Optional","Optional","–","–","–","–","–","–"]
["Extended wear air package ","Optional","Optional","Optional","Optional","–","–","–","–","–","–"]
["Packer or gauge wheel deduct ","_","_","_","_","_","_","_","_","Optional","Optional"]
["Extended wear gauge wheel  ","_","_","_","_","_","_","_","_","Optional","Optional"]
["Tank mounted weight scales ","_","_","_","_","_","_","_","_","Optional","Optional"]
["In-tank and rear-view cameras ","_","_","_","_","_","_","_","_","Optional","Optional"]
["Tank fill lighting package ","_","_","_","_","_","_","_","_","Optional","Optional"]
["Intelliview™ IV Display ","_","_","_","_","_","_","_","_","Optional","Optional"]
["     * Additional horsepower is required to tow and operate the air cart. Minimum requirements are a starting point only and should be increased based on operating conditions in the field, road transport conditions, and other implements that are used with the drill.  See product brochure for full specifications and options. "]