{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":4,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[null,"SP310F","SP370F","SP410F"]
["Specifications"]
["Engine ","FPT® NEF 6 / 6.7 Liter Tier 4B","FPT® Cursor 9 / 8.7 Liter Tier 4B","FPT® Cursor 9 / 8.7 Liter Tier 4B"]
["Rated Power (hp (kW)) ","285 (212)","328 (244)","382 (284)"]
["Power Bulge (hp (kW)) ","310 (231)","369 (275)","412 (307)"]
["Fuel Tank Capacity (gal. (L)) ","150 (568)","150 (568)","150 (568)"]
["DEF Tank Capacity (gal. (L)) ","24 (91)","24 (91)","24 (91)"]
["Transmission ","Hydrostatic drive with electronic controlled single Danfoss 165 cc, H1 series heavy duty pump","Hydrostatic drive with electronic controlled Danfoss H1 series heavy-duty twin 130 cc pumps","Hydrostatic drive with electronic controlled Danfoss H1 series heavy-duty twin 130 cc pumps"]
["Speed Range ","Full range with 4 user defined speed ranges","Full range with 4 user defined speed ranges","Full range with 4 user defined speed ranges"]
["Crop Clearance (in. (cm)) ","72 - 78 (182.88 - 198.12) (Variable height)","74 or 76 (187.96 or 193.04)","74 or 76 (187.96 or 193.04)"]
["Tank Material ","1000 gal (3785 L) Poly or Stainless Steel - 1200 gal (4542 L) Stainless Steel","Stainless Steel","Stainless Steel"]
["Tank Capacity (gal. (L)) ","1000 or 1200 (3785 or 4542)","1200, 1400 or 1600 (4542, 5300 or 6056)","1200, 1400 or 1600 (4542, 5300 or 6056)"]
["Rinse System ","Standard electric controls or optional Auto Rinse 150 gal. (568 L) poly tank with 2 in. (5.08 cm) fill connection","Standard electric controls or optional Auto Rinse 150 gal. (568 L) poly tank with 2 in. (5.08 cm) fill connection","Standard electric controls or optional Auto Rinse 150 gal. (568 L) poly tank with 2 in. (5.08 cm) fill connection"]
["Mono Boom Width (ft. (m)) ","90/60, 100/60 or 120/70 (27.4/18.3, 30.5/18.2 or 36.6/21.3)","90/60, 100/60 or 120/70 (27.4/18.3, 30.5/18.2 or 36.6/21.3)","90/60, 100/60 or 120/70 (27.4/18.3, 30.5/18.2 or 36.6/21.3)"]
["Truss Boom Width (ft. (m)) ","120/73, 132/73 or 135/73 (36.6/22.3, 40.2/22.3 or 41.1/22.3)","120/73, 132/73 or 135/73 (36.6/22.3, 40.2/22.3 or 41.1/22.3)","120/73, 132/73 or 135/73 (36.6/22.3, 40.2/22.3 or 41.1/22.3)"]
["Spray-Air Boom Width (ft. (m)) ","90, 100 or 120 (27.4, 30.4 or 36.6)","90, 100 or 120 (27.4, 30.4 or 36.6)","90, 100 or 120 (27.4, 30.4 or 36.6)"]
["Nozzle Bodies ","3+1 Way Turret / 5 Way Turret / IntelliSpray with 3+1 Turret","3+1 Way Turret / 5 Way Turret / IntelliSpray with 3+1 Turret","3+1 Way Turret / 5 Way Turret / IntelliSpray with 3+1 Turret"]
["Shipping Height (in. (cm)) ","153 (388.6)","154 (391)","154 (391)"]
["Shipping Width Mono Boom (in. (cm)) ","163 (414)","145 (368)","145 (368)"]
["Shipping Width Truss Boom (in. (cm)) ","183 (464.8)","173 (439.4)","173 (439.4)"]