{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[[58,0,58,7]]}
[]
[null,"TS6.110","TS6.120","TS6.120 High Clearance","TS6.130","TS6.140"]
["Power"]
["Engine Type ","4 cylinder, 16 valve, high pressure common rail, air-to-air intercooled turbo diesel","4 cylinder, 16 valve, high pressure common rail, air-to-air intercooled turbo diesel","4 cylinder, 16 valve, high pressure common rail, air-to-air intercooled turbo diesel","4 cylinder, 16 valve, high pressure common rail, air-to-air intercooled turbo diesel","4 cylinder, 16 valve, high pressure common rail, air-to-air intercooled turbo diesel"]
["Engine make / model ","Fiat Powertrain Industrial / FPT NEF","Fiat Powertrain Industrial / FPT NEF","Fiat Powertrain Industrial / FPT NEF","Fiat Powertrain Industrial / FPT NEF","Fiat Powertrain Industrial / FPT NEF"]
["Engine displacement (cu. in. (L)) ","274 (4.5)","274 (4.5)","274 (4.5 )","274 (4.5)","274 (4.5)"]
["Rated engine horsepower @ 2200 RPM ","110","119","119","130","139"]
["Rated PTO horsepower ","92","102","102","112","118"]
["Emissions certification ","Tier 4B/Final","Tier 4B/Final","Tier 4B/Final","Tier 4B/Final","Tier 4B/Final"]
["Fuel Tank Capacity (gal. (L)) ","57.5 (217.6)","57.5 (217.6)","57.5 (217.6)","57.5 (217.6)","57.5 (217.6)"]
["DEF (AdBlue®) Tank Capacity (gal. (L)) ","7.9 (30)","7.9 (30)","7.9 (30)","7.9 (30)","7.9 (30)"]
["Electrical System"]
["Alternator amps ","120","120","120","120","120"]
["Battery ","12 volt w/950 CCA","12 volt w/950 CCA","12 volt w/ 950 CCA","12 volt w/950 CCA","12 volt w/950 CCA"]
["Transmission"]
["Base transmission ","8x8 synchronized hydraulic shuttle with left hand shuttle","8x8 synchronized hydraulic shuttle with left hand shuttle","8x8 synchronized with left hand controlled mechanical shuttle","8x8 synchronized hydraulic shuttle with left hand shuttle","8x8 synchronized hydraulic shuttle with left hand shuttle"]
["Optional transmission ","8x8 synchronized mechanical shuttle with left hand shuttle","8x8 synchronized mechanical shuttle with left hand shuttle","8x8 synchronized with left hand controlled hydraulic shuttle","8x8 synchronized mechanical shuttle with left hand shuttle","8x8 synchronized mechanical shuttle with left hand shuttle"]
["Premium transmission ","16x8 dual power synchronized hydraulic shuttle with left hand shuttle","16x8 dual power synchronized hydraulic shuttle with left hand shuttle","–","16x8 dual power synchronized hydraulic shuttle with left hand shuttle","16x8 dual power synchronized hydraulic shuttle with left hand shuttle"]
["Creeper option ","10:1 gear ratio","10:1 gear ratio","10:1 gear ratio","10:1 gear ratio","10:1 gear ratio"]
["Rear PTO & 3-Point Hitch"]
["PTO rpm ","540/1000","540/1000","540/1000","540/1000","540/1000"]
["3-point hitch ","Category II w/flex link ends","Category II w/flex link ends","Category II w/flex link ends","Category II w/flex link ends","Category II w/flex link ends"]
["Base, 3-point hitch ASAE lift capacity (lbs. (kg)) ","3,735 (1693)","3,735 (1693)","3,735 (1693)","3,735 (1693)","3,735 (1693)"]
["Option 3, 3-pt. ASAE lift capacity (lbs. (kg)) ","5,499 (2499)","5,499 (2499)","5,499 (2499)","5,499 (2499)","5,499 (2499)"]
["Option 2, 3-pt. ASAE lift capacity (lbs. (kg)) ","7,326 (3323)","7,326 (3323)","7,326 (3323)","7,326 (3323)","7,326 (3323)"]
["Hydraulic System"]
["System type ","Fixed displacement pumps (steering, implement, aux) with combining/diverter valve","Fixed displacement pumps (steering, implement, aux) with combining/diverter valve","Fixed displacement pumps (steering, implement, aux) with combining/diverter valve","Fixed displacement pumps (steering, implement, aux) with combining/diverter valve","Fixed displacement pumps (steering, implement, aux) with combining/diverter valve"]
["Hydraulic implement pump flow* (gpm (Lpm)) ","13 (49)","13 (49)","13 (49)","13 (49)","13 (49)"]
["Optional auxiliary hydraulic pump flow* (gpm (Lpm)) ","9 (34)","9 (34)","9 (34)","9 (34)","9 (34)"]
["Rear hydraulic remote valves* ","Deluxe closed center with flow control and quick connect couplers","Deluxe closed center with flow control and quick connect couplers","Deluxe closed center with flow control and quick connect couplers","Deluxe closed center with flow control and quick connect couplers","Deluxe closed center with flow control and quick connect couplers"]
["Axles"]
["Front standard 2WD adjustable tread width (in. (mm)) ","_","_","–","56 (1432) to 80 (2028)","56 (1432) to 80 (2028)"]
["Front HD 2WD adjustable tread width (in. (mm)) ","–","–","–","60 (1524) to 84 (2134)","60 (1524) to 84 (2134)"]
["Rear flange axle adjustable tread width (in. (mm)) ","64 (1620) to 80 (2028)","64 (1620) to 80 (2028)","–","64 (1620) to 80 (2028)","64 (1620) to 80 (2028)"]
["Rear bar axle adjustable tread width (in. (mm)) ","60 (1524) to 80 (2028)","60 (1524) to 80 (2028)","–","60 (1524) to 80 (2028)","60 (1524) to 80 (2028)"]
["Rear axle type ","–","–","External drop box final drive with internal wet brakes","–","–"]
["Front 4WD adjustable tread width (in. (mm)) ","–","61.4 (1,560) to 88.8 (2256)","–","61.4 (1,560) to 88.8 (2256)","61.4 (1,560) to 88.8 (2256)"]
["Rear 4WD adjustable tread width (in. (mm)) ","–","–","72 (1829) to 100 (2540)","–","–"]
["Ground clearance** (lowest part of front axle) (in. (mm)) ","–","–","25.25 (616)","–","–"]
["Weight**"]
["Weight (shipping, 4WD, cab, flange axle) (lbs. (kg)) ","11,200 (5080)","11,200 (5080)","11,883 (5390)","11,200 (5080)","11,200 (5080)"]
["Weight (shipping, 4WD, cab, bar axle) (lbs. (kg)) ","12,192 (5530)","12,192 (5530)","–","12,192 (5530)","12,192 (5530)"]
["Weight (shipping, 2WD, cab) (lbs. (kg)) ","–","–","–","9,921 (4500)","9,921 (4500)"]
["Weight (shipping, 4WD, ROPS, flange axle) (lbs. (kg)) ","–","10,362 (4700)","10,957 (4970)","–","10,362 (4700)"]
["Weight (shipping, 4WD, ROPS, bar axle) (lbs. (kg)) ","–","11,002 (4990)","–","–","11,002 (4990)"]
["Max. tractor weight (G.V.W.), Cab, 4WD (lbs. (kg)) ","17,196 (7800)","17,196 (7800)","17,196 (7800)","18,298 (8300)","18,298 (8300)"]
["Dimensions**"]
["Wheel base 4WD (Std. Duty Class 3) (in. (mm)) ","99.2 (2520)","99.2 (2520)","107.5 (2730)","–","–"]
["Wheel base 4WD (HD Class 3) (in. (mm)) ","–","–","–","103.9 (2640)","103.9 (2640)"]
["Wheel base 2WD standard duty (6 bolt hub) (in. (mm)) ","100.4 (2550)","100.4 (2550)","–","100.4 (2550)","100.4 (2550)"]
["Wheel base 2WD heavy duty (8 bolt hub) (in. (mm)) ","95.8 (2432)","95.8 (2432)","–","95.8 (2432)","95.8 (2432)"]
["Overall length 4WD w/ front weights (in. (mm)) ","184.7 (4690)","184.7 (4690)","192.9 (4900)","184.7 (4690)","184.7 (4690)"]
["Overall length 2WD w/ front weights (in. (mm)) ","–","–","–","184.5 (4687)","184.5 (4687)"]
["Height to top of cab (in. (mm)) ","110.2 (2800)","110.2 (2800)","–","110.2 (2800)","110.2 (2800)"]
["Height to top of ROPS (in. (mm)) ","–","–","128.9 (3275)","117.3 (2980)","117.3 (2980)"]
["Height to top of exhaust (in. (mm)) ","109.8 (2790)","109.8 (2790)","121.4 (3085)","109.8 (2790)","109.8 (2790)"]
["Available Offering Configurations"]
["Available Offering Configurations ","MFD only, Cab only","MFD only, ROPS or Cab","MFD only, ROPS only","2WD or MFD, Cab only","2WD or MFD, ROPS (with MFD only) or Cab"]
["            *Oil flow at the remote couplers will be 10% to 15% less than pump flow        \n**Dimensions shown are with 18.4-38 R1 rear tires and 14.9-28 R1 4WD front tires or 10:00-16 2WD front tires​"]