{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":56,"n_cols":7,"rows_kept":56,"cut":false,"hidden":false,"merged":[]}
[]
[null,"WORKMASTER™ 25S Open-Air + 100LC Loader","WORKMASTER™ 25S Open-Air + 100LC Loader + 160GMS Mower","WORKMASTER™ 25S Open-Air + 100LC Loader + 905GBL Backhoe","WORKMASTER™ 25S Open-Air + 160GMS Mower","WORKMASTER™ 25S Cab + 100LC Loader","WORKMASTER™ 25S Cab + 100LC Loader + 160GMS Mower"]
["Engine"]
["Emissions Level ","T4B Final","T4B Final","T4B Final","T4B Final","T4B Final","T4B Final"]
["Gross horsepower (hp (kW)) ","24.7 (18.4)","24.7 (18.4)","24.7 (18.4)","24.7 (18.4)","24.7 (18.4)","24.7 (18.4)"]
["Rated speed (rpm) ","3000","3000","3000","3000","3000","3000"]
["No. of cylinders ","3","3","3","3","3","3"]
["Aspiration ","Natural","Natural","Natural","Natural","Natural","Natural"]
["Displacement (cu. in. (L)) ","77.3 (1.26)","77.3 (1.26)","77.3 (1.26)","77.3 (1.26)","77.3 (1.26)","77.3 (1.26)"]
["Alternator (amps) ","50","50","50","50","50","50"]
["Fuel Tank (gal. (L)) ","6.6 (25)","6.6 (25)","6.6 (25)","6.6 (25)","6.6 (25)","6.6 (25)"]
["PTO"]
["PTO horsepower (hp (kW)) ","17.2 (12.8)","17.2 (12.8)","17.2 (12.8)","17.2 (12.8)","17.2 (12.8)","17.2 (12.8)"]
["PTO speed (rpm) ","540","540","540","540","540","540"]
["PTO type ","Independent Electro-Hydraulic Engagement","Independent Electro-Hydraulic Engagement","Independent Electro-Hydraulic Engagement","Independent Electro-Hydraulic Engagement","Independent Electro-Hydraulic Engagement","Independent Electro-Hydraulic Engagement"]
["Mid-PTO ","Standard","Standard","Standard","Standard","Standard","Standard"]
["Mid-PTO speed (rpm) ","2500","2500","2500","2500","2500","2500"]
["Transmission"]
["Type/Control -  Choice 1 ","2 Range Hydrostatic/Dual Pedal","2 Range Hydrostatic/Dual Pedal","2 Range Hydrostatic/Dual Pedal","2 Range Hydrostatic/Dual Pedal","2 Range Hydrostatic/Dual Pedal","2 Range Hydrostatic/Dual Pedal"]
["Type/Control -  Choice 2 ","N/A","N/A","N/A","N/A","N/A","N/A"]
["Maximum forward speed (mph (kph)) ","9.1 (14.7)","9.1 (14.7)","9.1 (14.7)","9.1 (14.7)","9.1 (14.7)","9.1 (14.7)"]
["Cruise control ","Standard HST","Standard HST","Standard HST","Standard HST","Standard HST","Standard HST"]
["Gear/shuttle type ","Synchro","Synchro","Synchro","Synchro","Synchro","Synchro"]
["Rear diff-lock engagement ","Mechanical","Mechanical","Mechanical","Mechanical","Mechanical","Mechanical"]
["Brake type ","Wet, Multi-Disc","Wet, Multi-Disc","Wet, Multi-Disc","Wet, Multi-Disc","Wet, Multi-Disc","Wet, Multi-Disc"]
["Hydraulics & 3-Point"]
["Implement hydraulic flow (gpm (Lpm)) ","4.6 (17.4)","4.6 (17.4)","4.6 (17.4)","4.6 (17.4)","4.6 (17.4)","4.6 (17.4)"]
["Steering hydraulic flow (gpm (Lpm)) ","2.1 (8)","2.1 (8)","2.1 (8)","2.1 (8)","2.1 (8)","2.1 (8)"]
["Total Flow (gpm (Lpm)) ","6.7 (25.4)","6.7 (25.4)","6.7 (25.4)","6.7 (25.4)","6.7 (25.4)","6.7 (25.4)"]
["Remote Valves ","1 Opt.","1 Opt.","1 Opt.","1 Opt.","1 Opt.","1 Opt."]
["3-point hitch ","Chain Type Stabilizers /Fixed Link Ends","Chain Type Stabilizers /Fixed Link Ends","Chain Type Stabilizers /Fixed Link Ends","Chain Type Stabilizers /Fixed Link Ends","Chain Type Stabilizers /Fixed Link Ends","Chain Type Stabilizers /Fixed Link Ends"]
["3-point lift capacity @ ball ends (lbs. (kg)) ","992 (450)","992 (450)","992 (450)","992 (450)","992 (450)","992 (450)"]
["3-point lift capacity @ 24 in. (610 mm) behind ball ends (lbs. (kg)) ","728 (330)","728 (330)","728 (330)","728 (330)","728 (330)","728 (330)"]
["3-point linkage category ","I ","I ","I ","I ","I ","I "]
["Front Axle Options"]
["Two-Wheel Drive ","N/A","N/A","N/A","N/A","N/A","N/A"]
["Four-Wheel Drive ","Standard","Standard","Standard","Standard","Standard","Standard"]
["Dimensions/Weight"]
["Wheelbase (in. (mm)) ","56.1 (1425)","56.1 (1425)","56.1 (1425)","56.1 (1425)","56.1 (1425)","56.1 (1425)"]
["Length (in. (mm)) ","97.4 (2473)","97.4 (2473)","97.4 (2473)","97.4 (2473)","97.4 (2473)","97.4 (2473)"]
["Width (in. (mm)) ","46.7 (1187)","46.7 (1187)","46.7 (1187)","46.7 (1187)","46.7 (1187)","46.7 (1187)"]
["Height (top of ROPS or Cab) (in. (mm)) ","87.4 (2220)","87.4 (2220)","87.4 (2220)","87.4 (2220)","87.4 (2220)","87.4 (2220)"]
["Weight (lbs. (kg)) ","1444 (655)","1444 (655)","1444 (655)","1444 (655)","1805 (819)","1805 (819)"]
["100LC Loader"]
["Lift Capacity (max height) (lbs. (kg)) ","1005 (456)","1005 (456)","1005 (456)","–","1005 (456)","1005 (456)"]
["Lift Height  (in. (mm)) ","72 (1829)","72 (1829)","72 (1829)","–","72 (1829)","72 (1829)"]
["Bucket ","50 in. (1270 mm) /SSL QA","50 in. (1270 mm) /SSL QA","50 in. (1270 mm) /SSL QA","–","50 in. (1270 mm) /SSL QA","50 in. (1270 mm) /SSL QA"]
["Weight  (lbs. (kg)) ","363 (165)","363 (165)","363 (165)","–","363 (165)","363 (165)"]
["160GMS Mower"]
["Cutting Width (in. (mm)) ","–","60 (1524)","–","60 (1524)","–","60 (1524)"]
["No. of Blades ","–","3","–","3","–","3"]
["Weight (lbs. (kg)) ","–","285 (129)","–","285 (129)","–","285 (129)"]
["905GBL Backhoe"]
["Digging Depth (in. (mm)) ","–","–","79.4 (2017)","–","–","–"]
["Bucket (in. (mm)) ","–","–","9 (229)","–","–","–"]
["Weight (lbs. (kg)) ","–","–","707 (321)","–","–","–"]