{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":61,"n_cols":2,"rows_kept":61,"cut":false,"hidden":false,"merged":[[60,0,60,3]]}
[]
[null,"TC5.30"]
["High-Capacity grain header"]
["Cutting width (m/ft) ","4.57/15"]
["Knife speed (cuts/min.) ",1150]
["Electric reel speed control ","Standard"]
["Hydraulic reel height control ","Standard"]
["Reel fore-aft control ","Manual"]
["Maize headers"]
["Heavy duty driveline (2HC powerbelt) ","Standard"]
["Rigid maize header ","5 row"]
["Rotary dividers ","–"]
["Cab"]
["Mechanically suspended seat ","Standard"]
["Instructor’s seat ","Optional"]
["Air-conditioning ","Standard"]
["Remote controls for header, threshing and unloading engagement ","Standard"]
["Cab heating ","Optional"]
["Threshing drum"]
["Width (mm) ",1300]
["Diameter (mm) ",607]
["Speed range (rpm) ","387 - 1012"]
["Electric drum speed control ","Standard"]
["Drum concave"]
["Area (m²) ",0.79]
["Number of bars ",14]
["Angle of wrap (degrees) ",111]
["Concave adjustment ","Manual"]
["Rotary Separator"]
["Rotary Separator ","Optional"]
["Diameter (m) ",0.605]
["Speed (rpm) ","760 or 400"]
["Concave area (including rake) (m²) ",0.83]
["Multi-Thresh™ concave ","Standard"]
["Strawwalkers"]
["Number ",5]
["Separation area with Rotary Separator (m²) ",4.5]
["Separation area (less Rot. Sep.) (m²) ",5.3]
["Cleaning"]
["Total sieve area under wind control (m²) ",3.97]
["Double Cascade cleaning shoe with extra pre-sieve ","Standard"]
["Cleaning fan speed range (rpm) ","325 to 927"]
["Cleaning fan speed control ","Manual"]
["Graintank"]
["Volume (l) ",3500]
["Unload capacity (l/sec) ",65]
["Engine"]
["Displacement (l) ",5.9]
["Emission level ","Tier 3"]
["Injection system ","Mechanical injectors"]
["Gross power ECE R120 (2000 rpm) [kW/hp(CV)] ","96,35/131"]
["Air compressor kit ","Optional"]
["Fuel tank capacity (l) ",300]
["Transmission"]
["Traction ","Mechanical"]
["Speeds ","4 forward, 1 reverse"]
["Ground speed (km/h) ",25]
["Tracks ","Optional"]
["Front TW 18.4-30 14PR - Rear SW 9.00-16 16PR ","Standard"]
["Front TW 23.1-26-14PR-TD0 - Rear SW 12.0/75-18 12PR TR-03 ","Optional"]
["\n"]