{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":42,"n_cols":3,"rows_kept":42,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3230 TX Super - 2WD","3230 TX Super - 4WD"]
["Engine"]
["Engine Model ","T-IIIA, Simpson 325.5","T-IIIA, Simpson 325.5"]
["Engine Type ","Naturally Aspirated","Naturally Aspirated"]
["Engine Power ","33.83kW (45 HP)","33.83kW (45 HP)"]
["Rated RPM ",2200,2200]
["Air Cleaner"]
["Air Cleaner Type ","Oil bath type with Pre-cleaner","Oil bath type with Pre-cleaner"]
["Transmission"]
["Clutch ","Single Clutch/Double Clutch with IPTO lever*","Single/Double Clutch with IPTO lever*"]
["Type ","Constant Mesh AFD Side Shift","Constant Mesh AFD Side Shift"]
["Gear Box ","8F+2R & 8F+8R*","8F+8R & 8F+2R*"]
["PTO"]
["PTO Type ","Eptraa PTO - 540S, 540E*, Reverse PTO & GSPTO","Eptraa PTO - 540S, 540E*, Reverse PTO & GSPTO"]
["PTO HP ","41 HP (30.57 kW)","41 HP (30.57 kW)"]
["Hydraulics"]
["Lift Capacity ","1800 kg High Precision Hydraulic","1800 kg High Precision Hydraulic"]
["Lift-O-Matic ","Yes","Yes"]
["Rear Axle"]
["Rear Axle Type ","Straight Axle Planetary Drive","Straight Axle Planetary Drive"]
["Brakes"]
["Brake Type ","Oil Immersed Multi Disc Brake","Oil Immersed Multi Disc Brake"]
["Steering\t"]
["Information ","Power Steering","Power Steering"]
["Tyre"]
["Front ","6 in x 16 in (152.4 mm x 406.4 mm),\n6.5 in x 16 in (165.1 mm x 406.4 mm)*","8 in x 18 in (203.2 mm x 457.2 mm) - STS Axle,\n8.3 in x 24 in (210.82 mm x 609.6 mm) - MHD Axle,\n9.5 in x 24 in (241.3 mm x 609.6 mm) - MHD Axle"]
["Rear ","13.6 in x 28 in (345.44 mm x 711.2 mm),\n14.9 in x 28 in (378.46 mm x 711.2 mm)*","13.6 in x 28 in (345.44 mm x 711.2 mm),\n14.9 in x 28 in (378.46 mm x 711.2 mm)*"]
["Electricals "]
["Battery & Alternator ","75 Ah & 35 Amp","75 Ah & 35 Amp"]
["Dimension"]
["Overall Length (mm) ",3330,3370]
["Width (mm) ",1790,1790]
["Height (mm) ",2350,2445]
["Wheelbase (mm) ",1900,2000]
["Ground Clearance (mm) ",395,360]
["Weight (kg) ",1873,2150]
["Fuel Tank Capacity (L) ",46,46]
["Additional Features"]
["Information ","Heavy Duty Front Axle Support, Softek Clutch, Multisensing with DRC Valve, Tipping Trailer Pipe, Neutral Safety Switch, Clutch Safety Lock, Antiglare Rear View Mirror, Semi Flat Platform, Polymer Fuel Tank","Heavy Duty Front Axle Support, Deluxe Driver Seat, Multisensing with DRC Valve, Tipping Trailer Pipe, Neutral Safety Switch, Clutch Safety Lock, Antiglare Rear View Mirror, Semi Flat Platform, Polymer Fuel Tank, Paddy Special - Double Metal Face Sealing"]
["Optional Features"]
["Information ","Synchro Shuttle 8F*8R, Remote Valve, Economy PTO, Double Clutch with IPTO lever, 90 kg HD Front Bumper, Rear weight (32 kg each side), Potato Special Axle 48\" & Paddy Special - Double Metal Face Sealing, Deluxe Driver Seat","Double Clutch with IPTO lever, Synchro Shuttle 8F*8R, Economy PTO, HI-Lug Tyre, 55kg FWC, Rear weight (32 kg each side)"]