{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":39,"n_cols":3,"rows_kept":39,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3630 TX Super Plus+ 2WD","3630 TX Super Plus+ 4WD"]
["Engine"]
["Engine Model ","FPT S8000 series","FPT S8000 series"]
["Engine Type ","Naturally Aspirated","Naturally Aspirated"]
["Engine Power ","36.94 kW (49.5 HP)","36.94 kW (49.5 HP)"]
["Rated RPM ",2100,2100]
["Air Cleaner"]
["Air Cleaner Type ","Oil Bath Type with Pre-Cleaner","Oil Bath Type with Pre-Cleaner"]
["Transmission"]
["Clutch ","Double Clutch with Independent PTO Clutch Lever","Double Clutch with Independent PTO Clutch Lever"]
["Gear Box ","8F+2R/12F+3R Creeper*/12F+3R UG*, Constant Mesh/Partial Synchro Mesh","8F+2R/12F+3R Creeper*/12F+3R UG*, Constant Mesh/Partial Synchro Mesh"]
["PTO"]
["PTO Type ","540 + GSPTO/ RPTO (RPTO with UG Gear Box Only)","540 + GSPTO/ RPTO (RPTO with UG Gear Box Only)"]
["PTO HP ","46 HP (34.3 kW)","46 HP (34.3 kW)"]
["Hydraulics"]
["Lift Capacity ","Sensomatic24 Hydraulic (1700/2000* kg)","Sensomatic24 Hydraulic (1700/2000* kg)"]
["Lift-O-Matic with DRC & Isolator Valve ","Yes","Yes"]
["Rear Axle"]
["Rear Axle Type ","Outboard Reduction","Outboard Reduction"]
["Brakes"]
["Brake Type ","Real Oil Immersed Multi Disk Brake","Real Oil Immersed Multi Disk Brake"]
["Steering"]
["Information ","Power Steering","Power Steering"]
["Tyre"]
["Front ","7.5 in x 16 in (190.5 mm x 406.4 mm)","9.5 in x 24 in (241.3 mm x 609.6 mm)"]
["Rear ","16.9 in x 28 in (429.26 mm x 711.2 mm)","16.9 in x 28 in (429.26 mm x 711.2 mm)"]
["Electricals"]
["Information ","88 Ah Battery & 45 Amp Alternator","88 Ah Battery & 45 Amp Alternator"]
["Dimension"]
["Overall Length (mm) ",3465,3440]
["Width (mm) ",1815,1840]
["Height (mm) ",2390,2430]
["Wheelbase (mm) ",2040,1920]
["Ground Clearance (mm) ",445,390]
["Weight (kg) ",2180,2460]
["Fuel Tank Capacity (L) ",60,60]
["Factory Fitted Options\t"]
["Information ","Clear-lens Head Lamp with DRL, LED Fender Lamps, Softek Clutch with Safety lock, 55 kg Front Weight Carrier, Lift-O-matic with Height Limiter, ROPS with Fiber Canopy,Remote Valve, Double Metal Face Sealing, New Side Muffler, Heat Guards, Improved wider platform","Clear-lens Head Lamp with DRL, LED Fender Lamps, Softek Clutch with Safety lock, 55 kg Front Weight Carrier, Lift-O-matic with Height Limiter, ROPS with Fiber Canopy,Remote Valve, Double Metal Face Sealing, New Side Muffler, Heat Guards, Improved wider platform"]