{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":3,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
[]
[null,"5630 TX Plus TREM-IV 2WD","5630 TX Plus TREM-IV 4WD"]
["Engine"]
["Engine Model ","FPT S8000 series 12 Valve HPCR Engine","FPT S8000 series 12 Valve HPCR Engine"]
["Engine Type ","High Pressure Common Rail (TREM IV)","High Pressure Common Rail (TREM IV)"]
["Engine Power ","55 kW (75 HP Cat.)","55 kW (75 HP Cat.)"]
["Rated RPM ",2300,2300]
["Air Cleaner"]
["Air Cleaner Type ","8 inch (0.20 m) Dual Element, Dry Type","8 inch (0.20 m) Dual Element, Dry Type"]
["Transmission"]
["Clutch ","Double Clutch with Independent Clutch Lever","Double Clutch with Independent Clutch Lever"]
["Gear Box ","12F+3R Creeper*/12F+3R UG*, Partial Synchro Mesh","12F+3R Creeper*/12F+3R UG*, Partial Synchro Mesh"]
["PTO"]
["PTO Type ","540 + GSPTO/ RPTO (RPTO with UG Gear Box Only)","540 + GSPTO/ RPTO (RPTO with UG Gear Box Only)"]
["PTO HP ","69 HP (51.45 kW)","69 HP (51.45 kW)"]
["Hydraulics"]
["Lift Capacity ","Sensomatic24 Hydraulic with 2000 Kg Lift capacity","Sensomatic24 Hydraulic with 2000 Kg Lift capacity"]
["Lift-O-Matic Height Limiter with DRC & Isolator Valve ","Yes","Yes"]
["Rear Axle"]
["Rear Axle Type ","Heavy Duty Hub Reduction","Heavy Duty Hub Reduction"]
["Brakes"]
["Brake Type ","Oil Immersed Multi Disk Brake","Oil Immersed Multi Disk Brake"]
["Steering\t"]
["Information ","Power Steering","Power Steering"]
["Tyre"]
["Front ","6.5 in x 20 in (165.1 mm x 508 mm),\n7.5 in x 16 in (190.5 mm x 406.4 mm)*","12.4 in x 24 in (314.96 mm x 609.6 mm)"]
["Rear ","18.4 in x 30 in (467.36 mm x 762 mm)","18.4 in x 30 in (467.36 mm x 762 mm)"]
["Electricals \t"]
["Information ","100 Ah Battery & 55 Amp Alternator","100 Ah Battery & 55 Amp Alternator"]
["Dimension"]
["Overall Length (mm) ",3780,3780]
["Width (mm) ",2000,2000]
["Height (mm) ",2600,2600]
["Wheelbase (mm) ",2065,2045]
["Ground Clearance (mm) ",530,435]
["Weight (kg) ",2635,2835]
["Fuel Tank Capacity (L) ",70,70]
["Additional Features\t"]
["Information ","Multiple Engine Modes, DRL, Telescopic Stabilizer","Multiple Engine Modes, DRL, Telescopic Stabilizer"]
["Optional Features\t"]
["Information ","\"Remote Valve upto 4 Ports, Swinging Drawbar, ROPS\nwith Canopy, Front Fender\"","\"Remote Valve upto 4 Ports, Swinging Drawbar, ROPS\nwith Canopy, Front Fender\""]