{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
[null,"BC5060"]
["Specifications"]
["Pickup Width/Lift Type ","1.8 m (72 inch)/ Hydraulic"]
["Number of  Pickup Teeth/Tooth Bars ","110/ 05"]
["Knotter Type/ Number ","Twine-Standard / 02"]
["Picku-up Lift ","Hydraulic"]
["Twine Carrying Capacity ","6 Twine Balls"]
["Feeding System ","Packer fork + 2 Paired Rotors"]
["Bale Chamber Size ","0.356 m x 0.457 m (14 inch x 18 inch)"]
["Bale Length ","0.305m to 1.321 m (12 inch to 52 inch)"]
["Plunger Speed ","93 Stroke Per Minute"]
["Densification Mechanism ","Hydroformatic"]
["Required Tractor Power ","50 HP"]
["Recommended New Holland Tractors ","NH3600-2, NH3630 Super Plus, NH3630 TX, NH6010"]