{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
[null,"BC5060"]
["विशिष्टताएँ"]
["पिकअप चौड़ाई/लिफ्ट टाइप  ","1.8 m (72 इंच) / हाइड्रॉलिक"]
["पिकअप टीथ/टूथ बार की संख्या  ","110/ 05"]
["नॉटर का प्रकार/संख्या  ","ट्वाइन-मानक / 02"]
["पिकू-अप लिफ्ट  ","हाइड्रॉलिक"]
["ट्वाइन ले जाने की क्षमता  ","6 ट्वाइन बॉल्स"]
["फीडिंग सिस्टम  ","पैकर फोर्क + 2 युग्मित रोटर"]
["बेल चैम्बर का आकार  ","0.356 m x 0.457 m (14 इंच x 18 इंच)"]
["बेल की लंबाई  ","0.305 m से 1.321 m (12 इंच से 52 इंच)"]
["प्लंजर स्पीड  ","93 स्ट्रोक प्रति मिनट"]
["सघनीकरण तंत्र  ","हाइड्रोफॉर्मेटिक"]
["आवश्यक ट्रैक्टर पावर  ","50 HP"]
["अनुशंसित न्यू हॉलैंड ट्रैक्टर  ","NH3600-2, NH3630 सुपर प्लस, NH3630 TX"]