{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":70,"n_cols":6,"rows_kept":70,"cut":false,"hidden":false,"merged":[[69,0,69,7]]}
[]
[null," T5.110 DYNAMIC COMMAND™"," T5.120 DYNAMIC COMMAND™"," T5.130 DYNAMIC COMMAND™"," T5.140 DYNAMIC COMMAND™","T5.140 AUTO COMMAND™"]
["Engine*"]
["Engine* ","FPT NEF","FPT NEF","FPT NEF","FPT NEF","FPT NEF"]
["No. of cylinders / Capacity / Valves / Compliant emissions regulations ","4 / 4485 / 4 / Stage V ECOBlue™ HI-eSCR 2 system","4 / 4485 / 4 / Stage V ECOBlue™ HI-eSCR 2 system","4 / 4485 / 4 / Stage V ECOBlue™ HI-eSCR 2 system","4 / 4485 / 4 / Stage V ECOBlue™ HI-eSCR 2 system","4 / 4485 / 4 / Stage V ECOBlue™ HI-eSCR 2 system"]
["Max. horsepower - ISO TR14396- ECE R120 [kW/hp(CV)] ","81/110","88/120","96/130","103/140","103/140"]
["Rated horsepower (Rated speed @2200rpm) - ISO TR14396- ECE R120 [kW/hp(CV)] ","74/100","81/110","88/120","96/130","96/130"]
["Max. torque - ISO TR14396 (Nm) ","520@1300rpm","551@1300rpm","610@1300rpm","630@1300rpm","630@1300rpm"]
["Diesel tank capacity / AdBlue tank capacity (Litres) ","180 / 19","180 / 19","180 / 19","180 / 19","180 / 19"]
["Electrical 12 volt alternator Standard / Optional ","120 / 200","120 / 200","120 / 200","120 / 200","120 / 200"]
["Dynamic Command™ 8 step semi-powershift transmission"]
["Dynamic Command™ 8 step semi-powershift transmission (opt. 40kph ECO) ","Standard","Standard","Standard","Standard","–"]
["Min. speed / Max. speed @1650rpm (kph) ","0.216 / 40**","0.216 / 40","0.216 / 40","0.216 / 40","–"]
["Ground Speed Management II (GSM II) ","Optional","Optional","Optional","Optional","–"]
["Dynamic StartStop ","Standard","Standard","Standard","Standard","–"]
["CommandGrip™ and Basic Gear Display-DOG ","Standard","Standard","Standard","Standard","–"]
["IntelliView™ IV Plus colour monitor with ISO 11783 connector ","Optional","Optional","Optional","Optional","–"]
["Auto Command™ continuously variable transmission"]
["Auto Command™ Continuously Variable Transmission (opt. 40kph ECO) ","–","–","–","–","Standard"]
["Min. speed / Max. speed @1600rpm (kph) ","–","–","–","–","0.02 / 40"]
["Electronic park brake ","–","–","–","–","Standard"]
["Active StopStart function ","–","–","–","–","Standard"]
["CommandGrip and IntelliView™ IV Plus colour monitor with ISO 11783 connector ","–","–","–","–","Standard"]
["Standard Class 1.5 HD Front Axle"]
["Standard Class 1.5 HD Front Axle ","Standard","Standard","Standard","Standard","Standard"]
["Class 1.75 Front Axle ","Optional","Optional","Optional","Optional","Optional"]
["Terraglide™ front axle suspension ","Optional","Optional","Optional","Optional","Optional"]
["Terralock™ Auto Diff & Auto 4WD ","Standard","Standard","Standard","Standard","Standard"]
["Turning radius with 4WD / Terraglide™ suspended front axle (mm) ","4615","4615","4615","4615","4615"]
["PTO engine speed"]
["PTO engine speed at: 540 / 1000 (rpm) ","1938 / 1926","1938 / 1926","1938 / 1926","1938 / 1926","1938 / 1926"]
["PTO engine speed at: 540 / 540E / 1000 (rpm) ","1969 / 1546 / 1893","1969 / 1546 / 1893","1969 / 1546 / 1893","1969 / 1546 / 1893","1969 / 1546 / 1893"]
["PTO engine speed at: 540E / 1000 / 1000E (rpm) ","1546 / 1893 / 1621","1546 / 1893 / 1621","1546 / 1893 / 1621","1546 / 1893 / 1621","1546 / 1893 / 1621"]
["Ground Speed PTO ","Optional","Optional","Optional","Optional","Optional"]
["Auto PTO management ","Optional","Optional","Optional","Optional","Standard"]
["Front PTO (1000rpm) ","Optional","Optional","Optional","Optional","Optional"]
["Standard Hydraulic Main Pump 80Lpm flow / 200 bar Pump pressure"]
["Standard Hydraulic Main Pump 80Lpm flow / 200 bar Pump pressure ","Standard","Standard","Standard","Standard","–"]
["MegaFlow™ Hydraulic Main Pump 110Lpm flow / 200 bar Pump pressure ","Optional","Optional","Optional","Optional","Standard"]
["Standard Steering and services pump flow (Lpm / Bar) ","36.3 / 230","36.3 / 230","36.3 / 230","36.3 / 230","36.3 / 230"]
["Max. no. Deluxe rear valves with diverter fitted ","4 (Offering = 4 Mech. / 3 Mech. / 2 Electro + 2 Mech. / 3 Electro / 4 Electro)","4 (Offering = 4 Mech. / 3 Mech. / 2 Electro + 2 Mech. / 3 Electro / 4 Electro)","4 (Offering = 4 Mech. / 3 Mech. / 2 Electro + 2 Mech. / 3 Electro / 4 Electro)","4 (Offering = 4 Mech. / 3 Mech. / 2 Electro + 2 Mech. / 3 Electro / 4 Electro)","4 (Offering = 4 Mech. / 3 Mech. / 2 Electro + 2 Mech. / 3 Electro / 4 Electro)"]
["Max. no. mid mount valves ","3","3","3","3","3"]
["Advanced Joystick control (Forward / Reverse + Gear Change) ","Optional","Optional","Optional","Optional","Optional"]
["Electronic Draft Control (EDC)"]
["Electronic Draft Control (EDC) ","Standard","Standard","Standard","Standard","Standard"]
["Max. lift capacity at ball ends (kg) ","5500","5500","5500","5500","5500"]
["Front linkage lift capacity at ball ends (through the range) (kg) ","2250","2250","2250","2250","2250"]
["Four pillar 360° Horizon™ cab with FOPS - OECD Code 10 Level 1"]
["Four pillar 360° Horizon™ cab with FOPS - OECD Code 10 Level 1 ","Standard","Standard","Standard","Standard","Standard"]
["Low roof and Super High visibility roof hatch ","Optional","Optional","Optional","Optional","Optional"]
["Comfort Ride™ cab suspension ","Standard","Standard","Standard","Standard","Standard"]
["Automatic climate control ","Optional","Optional","Optional","Optional","Optional"]
["Comfort seat with seat belt ","Standard","Standard","Standard","Standard","Standard"]
["Dynamic Comfort™ seat with seat belt ","Optional","Optional","Optional","Optional","Optional"]
["Instructors seat with seat belt ","Optional","Optional","Optional","Optional","Optional"]
["Blue Power Pack Including Auto Comfort™ Active Climate Control heated seat with seat belt ","–","Optional","–","Optional","Optional"]
["4 halogen lighting pack ","Standard","Standard","Standard","Standard","Standard"]
["8 / 12 / 16 LED lighting pack ","Optional / Optional / Optional","Optional / Optional / Optional","Optional / Optional / Optional","Optional / Optional / Optional","Optional / Optional / Optional"]
["IntelliSteer® ","Optional","Optional","Optional","Optional","Optional"]
["Headland Turn Sequencing II (HTS II) ","Optional","Optional","Optional","Optional","Optional"]
["IntelliTurn™ with Headland Turn Sequencing II (HTS II) system ","Optional","Optional","Optional","Optional","Standard"]
["FieldOps™ ","Optional","Optional","Optional","Optional","Optional"]
["Dimensions"]
["Max. Overall length inc weight carrier to rear linkage (mm) ","4397","4397","4397","4397","4397"]
["Min. Width narrow / standard (mm) ","1888 / 2288","1888 / 2288","1888 / 2288","1888 / 2288","1888 / 2288"]
["Height from centre of rear axle to low profile / Standard cab (mm) ","1980 / 2100","1980 / 2100","1980 / 2100","1980 / 2100","1980 / 2100"]
["Wheelbase (mm) ","2490","2490","2490","2490","2490"]
["Minimum shipping weights (kg) ","5500","5500","5500","5500","5500"]
["Gross Vehicle Weight (kg) ","8800","8800","8800","8800","8800"]
["     * Developed by FPT Industrial              \n** @1600rpm"]