{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":128,"n_cols":6,"rows_kept":128,"cut":false,"hidden":false,"merged":[[127,0,127,7]]}
[]
[null," T5.80"," T5.90"," T5.100"," T5.110"," T5.120"]
["Engine*"]
["Engine* ","F5","F5","F5","F5","F5"]
["No. of Cylinders / Aspiration / Valves / Emission level ","4 / T / 4 / Stage V","4 / T / 4 / Stage V","4 / T / 4 / Stage V","4 / T / 4 / Stage V","4 / T / 4 / Stage V"]
["Fuel System - High Pressure Common Rail ","Standard","Standard","Standard","Standard","Standard"]
["Capacity (cm³) ",3600,3600,3600,3600,3600]
["Bore and Stroke (mm) ","99x102","99x102","99x102","99x102","99x102"]
["Approved Biodiesel blend ","B20**","B20**","B20**","B20**","B20**"]
["Max. horsepower (@1900rpm) - ISO TR14396 - ECE R120 [kW/hp(CV)] ","59/80","66/90","74/101","81/110","86/117"]
["Rated horsepower - ISO TR14396 - ECE R120 [kW/hp(CV)] ","59/80","66/90","74/101","81/110","86/117"]
["Rated engine speed (rpm) ",2300,2300,2300,2300,2300]
["Max. torque - ISO TR14396 (Nm@rpm) ","330@1300","380@1300","450@1300","490@1300","506@1300"]
["Torque rise (%) ",35,39,47,46,42]
["Horizontal exhaust ","Optional","Optional","Optional","Optional","Optional"]
["Vertical exhaust ","Standard","Standard","Standard","Standard","Standard"]
["Diesel tank capacity (Litres) ",129,129,129,129,129]
["Service interval (hours) ",600,600,600,600,600]
["Synchro Shuttle™ transmission [Optional Creeper (30kph / 40kph)]"]
["Synchro Shuttle™ transmission [Optional Creeper (30kph / 40kph)] ","Optional","Optional","Optional","–","–"]
["Number of gears (FxR) ","20x20","20x20","20x20","–","–"]
["Minimum speed (30kph / 40kph) (kph) ","0.09 / 0.11","0.09 / 0.11","0.09 / 0.11","–","–"]
["Gears in the 4-12kph working range ",4,4,4,"–","–"]
["Hydraulic Powershuttle transmission (30kph / 40kph)"]
["Hydraulic Powershuttle transmission (30kph / 40kph) ","Optional","Optional","Optional","Optional","Optional"]
["Number of gears (FxR) ","12x12","12x12","12x12","12x12","12x12"]
["Minimum speed (30kph / 40kph) (kph) ","1.81 / 2.15","1.81 / 2.15","1.81 / 2.15","1.81 / 2.15","1.81 / 2.15"]
["Gears in the 4-12kph working range ",6,6,6,6,6]
["Hydraulic Powershuttle transmission [Optional Creeper (30kph / 40kph)]"]
["Hydraulic Powershuttle transmission [Optional Creeper (30kph / 40kph)] ","Optional","Optional","Optional","Optional","Optional"]
["Number of gears (FxR) ","20x20","20x20","20x20","20x20","20x20"]
["Minimum speed (30kph / 40kph) (kph) ","0.25 / 0.30","0.25 / 0.30","0.25 / 0.30","0.25 / 0.30","0.25 / 0.30"]
["Gears in the 4-12kph working range ",6,6,6,6,6]
["Split Command™ transmission (30kph / 40kph)"]
["Split Command™ transmission (30kph / 40kph) ","Optional","Optional","Optional","Optional","Optional"]
["Number of gears (FxR) ","24x24","24x24","24x24","24x24","24x24"]
["Minimum speed (30kph / 40kph) (kph) ","0.56 / 0.69","0.56 / 0.69","0.56 / 0.69","0.56 / 0.69","0.56 / 0.69"]
["Gears in the 4-12kph working range ",12,12,12,12,12]
["Dual Command™ transmission (40kph)"]
["Dual Command™ transmission (40kph) ","Optional","Optional","Optional","Optional","Optional"]
["Number of gears (FxR) ","24x24","24x24","24x24","24x24","24x24"]
["Powershuttle lever with aggressiveness setting switch ","Standard","Standard","Standard","Standard","Standard"]
["Minimum speed (kph) ","2025-01-31","2025-01-31","2025-01-31","2025-01-31","2025-01-31"]
["Power Clutch ","Standard","Standard","Standard","Standard","Standard"]
["Gears in the 4-12kph working range ",12,12,12,12,12]
["Dual Command™ transmission [Optional Creeper (40kph)]"]
["Dual Command™ transmission [Optional Creeper (40kph)] ","Optional","Optional","Optional","Optional","Optional"]
["Number of gears (FxR) ","40x40","40x40","40x40","40x40","40x40"]
["Powershuttle lever with aggressiveness setting switch ","Standard","Standard","Standard","Standard","Standard"]
["Minimum speed (kph) ","0,17","0,17","0,17","0,17","0,17"]
["Power Clutch ","Standard","Standard","Standard","Standard","Standard"]
["Gears in the 4-12kph working range ",12,12,12,12,12]
["Electrical"]
["12 volt alternator standard / optional (Amps) ","120 / 200","120 / 200","120 / 200","120 / 200","120 / 200"]
["Standard battery capacity (CCA / Ah) ","800 / 100","800 / 100","961 / 132","962 / 132","962 / 132"]
["Axles"]
["4WD front axle ","Standard","Standard","Standard","Standard","Standard"]
["Large Heavy Duty class 1.5 front axle ","–","–","Optional","Optional","Standard"]
["SuperSteer™ front axle ","–","Optional","Optional","Optional","–"]
["Steering angle 4WD / SuperSteer™ (°) ","55 / –","55 / 76","55 / 76","55 / 76","55 / –"]
["Dynamic Front Fenders ","Optional","Optional","Optional","Optional","Optional"]
["Electro hydraulic 4WD engagement ","Standard","Standard","Standard","Standard","Standard"]
["Limited slip front diff. lock ","Standard","Standard","Standard","Standard","Standard"]
["Mechanical diff. lock engagement ","Standard","Standard","Standard","Standard","Standard"]
["Electro hydraulic diff. lock engagement ","Optional","Optional","Optional","Optional","Optional"]
["Turning radius 4WD / SuperSteer™ (mm) ","4235 / 3905","4235 / 3905","4235 / 3905","4235 / 3905","4235 / 3905"]
["Hydraulics"]
["Standard main pump flow / pressure @2300rpm (Lpm / Bar) ","48 / 190","48 / 190","48 / 190","48 / 190","48 / 190"]
["MegaFlow™ option main pump flow / pressure @2300rpm (Lpm / Bar) ","64 / 190","64 / 190","64 / 190","64 / 190","64 / 190"]
["Standard services pump flow / pressure @2300rpm (Lpm / Bar) ","28 / 170","28 / 170","28 / 170","28 / 170","28 / 170"]
["MegaFlow™ option services pump flow / pressure @2300rpm (Lpm / Bar) ","37 / 170","37 / 170","37 / 170","37 / 170","37 / 170"]
["Lift-O-Matic™ Plus system (MDC) ","Standard","Standard","Standard","Standard","Standard"]
["Electronic Draft Control (EDC)*** ","Optional","Optional","Optional","Optional","Optional"]
["Remote valves"]
["Type ","Deluxe","Deluxe","Deluxe","Deluxe","Deluxe"]
["Max. no. rear valves / diverter ","2025-03-01","2025-03-01","2025-03-01","2025-03-01","2025-03-01"]
["Max. no rear remote outlets ",8,8,8,8,8]
["Max. no. mid mount valves ",2,2,2,2,2]
["Max. no. mid mount outlets ",4,4,4,4,4]
["Mid mount joystick control ","Optional","Optional","Optional","Optional","Optional"]
["Linkage"]
["Rear linkage category ",2,2,2,2,2]
["Max. lift capacity at ball ends (kg) ",4400,4400,4400,4400,4400]
["Max. lift capacity through the range (610 mm behind ball ends) (kg) ",3900,3900,3900,3900,3900]
["Front linkage lift capacity at ball ends (through the range) (kg) ",1700,1700,1700,1700,1700]
["Front Loader Ready"]
["Front Loader Ready ","Optional","Optional","Optional","Optional","Optional"]
["Integrated loader joystick ","Optional","Optional","Optional","Optional","Optional"]
["PTO"]
["Mechanical PTO engagement**** ","Standard","Standard","Standard","Standard","Standard"]
["Servo Assisted PTO engagement***** ","Optional","Optional","Optional","Optional","Optional"]
["Electro hydraulic PTO engagement****** ","Optional","Optional","Optional","Optional","Optional"]
["Soft Start PTO activation****** ","Standard","Standard","Standard","Standard","Standard"]
["Engine speed at: 540 ",1938,1938,1938,1938,"–"]
["Engine speed at: 540 / 1000 ","1938 / 1926","1938 / 1926","1938 / 1926","1938 / 1926","1938 / 1926"]
["Engine speed at: 540 / 540E / 1000 ","1938 / 1535 / 1926","1938 / 1535 / 1926","1938 / 1535 / 1926","1938 / 1535 / 1926","1938 / 1535 / 1926"]
["Ground Speed ","Optional","Optional","Optional","Optional","Optional"]
["Front PTO (1000rpm) ","Optional","Optional","Optional","Optional","Optional"]
["Brakes"]
["Mechanical Park Lock ","Optional","Optional","Optional","Optional","Optional"]
["Hydraulic Trailer Brakes ","Optional","Optional","Optional","Optional","Optional"]
["Optional Pneumatic Tractor Brakes ","Optional","Optional","Optional","Optional","Optional"]
["Cab"]
["Suspended platform with rear mounted foldable ROPS ","Optional","Optional","Optional","Optional","Optional"]
["Optional FOPS protected canopy for ROPS ","Optional","Optional","Optional","Optional","Optional"]
["Deluxe VisionView™ cab with FOPS - OECD Code 10 Level 1 ","Standard","Standard","Standard","Standard","Standard"]
["Deluxe VisionView™ cab category level - EN 15695 ",2,2,2,2,2]
["High visibility roof hatch ","Optional","Optional","Optional","Optional","Optional"]
["Openable front windscreen ","Optional","Optional","Optional","Optional","Optional"]
["Rear window wiper / washer ","Optional","Optional","Optional","Optional","Optional"]
["Standard air suspension seat with seat belt ","Standard","Standard","Standard","Standard","Standard"]
["Deluxe air suspension 15° swivel seat with seat belt ","Optional","Optional","Optional","Optional","Optional"]
["Instructor seat with seat belt ","Optional","Optional","Optional","Optional","Optional"]
["Tilting steering column ","Optional","Optional","Optional","Optional","Optional"]
["Air conditioning ","Optional","Optional","Optional","Optional","Optional"]
["Air Recirculation Filters ","Standard","Standard","Standard","Standard","Standard"]
["MP3 Radio (with aux input socket) ","Optional","Optional","Optional","Optional","Optional"]
["Telescopic Shatterproof Mirrors ","Optional","Optional","Optional","Optional","Optional"]
["Fender mounted external PTO & Linkage controls*** ","Optional","Optional","Optional","Optional","Optional"]
["Performance Monitor with enhanced key pad and ISO 11786 connector ","Optional","Optional","Optional","Optional","Optional"]
["Cab monitor mounting bracket ","Optional","Optional","Optional","Optional","Optional"]
["Optimum Deluxe VisionView™ cab noise level - 77/311EEC (dB(A)) ",76,76,76,76,76]
["Factory Fit Rotating Beacons (1 / 2) ","Optional","Optional","Optional","Optional","Optional"]
["Weights"]
["Minimum unballasted / shipping weights: 4WD front axle with ROPS******* (kg) ",3245,3245,3245,3245,3245]
["Minimum unballasted / shipping weights: 4WD front axle with cab******** (kg) ",4030,4030,4030,4030,4030]
["4WD Max. permissible weight at 40kph Standard axle / Heavy Duty axle (kg) ",6200,6200,"6200 / 6500","6200 / 6500","6200 / 6500"]
["           * Developed by FPT Industrial              \n** Conditions Apply              \n*** Dual Command™ Cab models only              \n**** Synchro Shuttle™ ROPS models              \n***** Synchro Shuttle™ Cab models              \n****** Hydraulic Powershuttle and Dual Command™ models              \n******* Without FHPL/loader ready/TBV, with Shuttle transmission/1.0 STD front axle/small tyre option              \n******** Without FHPL/loader ready, with Powershuttle transmission/1.0 HD front axle/HTBV/small tyre option"]