{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":98,"n_cols":3,"rows_kept":98,"cut":false,"hidden":false,"merged":[[97,0,97,4]]}
[]
[null,"T5.90S","T5.100S"]
["Engine*"]
["Engine* ","F5C","F5C"]
["No. of Cylinders / Aspiration / Valves / Emission level ","4 / T / 4 / Stage V","4 / T / 4 / Stage V"]
["Fuel System - High Pressure Common Rail ","Standard","Standard"]
["Capacity (cm3) ","3600","3600"]
["Bore and Stroke (mm) ","102x110","102x110"]
["Approved Biodiesel blend ","B20**","B20**"]
["Max. horsepower (@1900rpm) - ISO TR14396 - ECE R120 [kW/hp(CV)] ","66/90","74/101"]
["Rated horsepower - ISO TR14396 - ECE R120 [kW/hp(CV)] ","66/90","74/101"]
["Rated engine speed (rpm) ","2300","2300"]
["Max. torque - ISO TR14396 (Nm@rpm) ","380@1300","450@1300"]
["Torque rise (%) ","40","47"]
["Vertical exhaust ","Standard","Standard"]
["Diesel tank capacity (Litres) ","129","129"]
["AdBlue tank capacity (Litres) ","10","10"]
["Service interval (hours) ","600","600"]
["Synchro Shuttle™ transmission (40kph)"]
["Synchro Shuttle™ transmission (40kph) ","Standard","Standard"]
["Number of gears (FxR) ","12x12","12x12"]
["Minimum speed (kph) ","0,91","0.91"]
["Synchro Shuttle™ transmission [Optional Creeper] (40kph)"]
["Synchro Shuttle™ transmission [Optional Creeper] (40kph) ","Optional","Optional"]
["Number of gears (FxR) ","20x20","20x20"]
["Minimum speed (kph) ","0,123","0.123"]
["Hydraulic Powershuttle transmission (40kph)"]
["Hydraulic Powershuttle transmission (40kph) ","Optional","Optional"]
["Number of gears (FxR) ","12x12","12x12"]
["Minimum speed (kph) ","0,91","0.91"]
["Hydraulic Powershuttle transmission [Optional Creeper] (40kph)"]
["Hydraulic Powershuttle transmission [Optional Creeper] (40kph) ","Optional","Optional"]
["Number of gears (FxR) ","20x20","20x20"]
["Minimum speed (kph) ","0,123","0.123"]
["Electrical"]
["12 volt alternator (Amps) ","120","120"]
["Standard battery capacity (CCA / Ah) ","800 / 143","800 / 143"]
["Axles"]
["4WD front axle ","Standard","Standard"]
["Heavy Duty class 1.0 front axle ","Standard","Standard"]
["Steering angle 4WD (°) ","55","55"]
["Dynamic Front Fenders ","Optional","Optional"]
["Limited slip front diff. lock ","Standard","Standard"]
["Mechanical diff. lock engagement ","Standard","Standard"]
["Electro hydraulic diff. lock engagement ","Optional","Optional"]
["Turning radius 4WD (mm) ","4235","4235"]
["Hydraulics"]
["Standard main pump flow / pressure @2300rpm (Lpm / Bar) ","48/190","48 / 190"]
["High flow option main pump flow / pressure @2300rpm (Lpm / Bar) ","64/190","64 / 190"]
["MegaFlow™ option main pump flow / pressure @2300rpm (Lpm / Bar) ","82/190","82 / 190"]
["Standard services pump flow / pressure @2300rpm (Lpm / Bar) ","28/190","28 / 190"]
["High flow option services pump flow/ pressure @2300rpm (Lpm / Bar) ","36/190","36 / 190"]
["MegaFlow™ option services pump flow / pressure @2300rpm (Lpm / Bar) ","37/190","37 / 190"]
["Lift-O-Matic™ system (MDC) ","Standard","Standard"]
["Remote valves"]
["Type ","Deluxe","Deluxe"]
["Max. rear valves ","3","3"]
["Max. no. rear remote outlets ","6","6"]
["Max. no. mid mount valves ","2","2"]
["Max. no. mid mount outlets ","4","4"]
["Mid mount joystick control ","Optional","Optional"]
["Linkage"]
["Rear linkage category ","2","2"]
["Max. lift capacity at ball ends (kg) ","4400","4400"]
["Max. lift capacity (OECD, 610mm behind ball ends) (kg) ","3700","3700"]
["Front linkage lift capacity at ball ends (through the range) (kg) ","1670","1600"]
["Front Loader Ready"]
["Front Loader Ready ","Optional","Optional"]
["Integrated loader joystick ","Optional","Optional"]
["PTO"]
["Mechanical PTO engagement ","Standard","Standard"]
["Soft Start PTO activation ","Optional","Optional"]
["Engine speed at (Synchro Shuttle™): 540 / 540E ","1938 / 1535","1938 / 1535"]
["Engine speed at (Synchro Shuttle™): 540 / 1000 ","1938 / 1926","1938 / 1926"]
["Engine speed at (Synchro Shuttle™): 540 / 540E / 1000 ","1938 / 1535 / 1926","1938 / 1535 / 1926"]
["Ground Speed ","Optional","Optional"]
["Front PTO (1000rpm) ","Optional","Optional"]
["Engine speed at (Powershuttle): 540 / 540E ","1938 / 1535","1938 / 1535"]
["Engine speed at (Powershuttle): 540 / 1000 ","1938 / 1926","1938 / 1926"]
["Engine speed at (Powershuttle): 540 / 540E / 1000 ","1938 / 1535 / 1926","1938 / 1535 / 1926"]
["Brakes"]
["Hydraulic Trailer Brakes ","Standard","Optional"]
["Optional Pneumatic Tractor Brakes ","Optional","Optional"]
["Cab"]
["Air conditioning / openable transparent hatch / sunroof / radio + speakers / instructor seat ","Standard","Standard"]
["Standard Mechanical suspension seat with seat belt & armrest ","Standard","Standard"]
["Optional Air suspension seat with seat belt & armrest ","Optional","Optional"]
["Tilting steering column ","Standard","Standard"]
["Air conditioning ","Standard","Standard"]
["Air Recirculation Filters ","Standard","Standard"]
["Telescopic Mirrors ","Optional","Optional"]
["Cab monitor mounting bracket ","Optional","Optional"]
["Cab Noise Level [dB(A)] ","77","77"]
["Factory Fit Rotating Beacon ","Optional","Optional"]
["Weights: Minimum unballasted / shipping weights"]
["4WD front axle with cab (kg) ","4000","4000"]
["4WD Max. permissible weight at 40kph / Heavy Duty axle (kg) ","6500","6500"]
["* Developed by FPT Industrial\n** Biodiesel blend must fully comply with the latest fuel specification EN14214:2009 and operation is in accordance with operator manual guidelines"]