{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":87,"n_cols":2,"rows_kept":87,"cut":false,"hidden":false,"merged":[[86,0,86,3]]}
[]
[null,"BigBaler 1290 High Density"]
["Bale dimensions"]
["Width (cm) ","120"]
["Height (cm) ","90"]
["Minimum / Maximum length (cm) ","100 / 300"]
["Tractor requirements"]
["Minimum PTO power ","Standard Packer 210hp / CropCutter 240hp"]
["PTO speed / type ","1000rpm / 20 spline shaft"]
["Standard hydraulic ","2 double acting valves, 1 single acting valve"]
["Load sensing remote hydraulics ","Power Beyond (pressure, return, LS), 1 x double acting valve"]
["Main Drive"]
["Mid gearbox type ","SmartShift™ 2 speed powershift"]
["Start up feature ","Smooth two-speed start-up, Smart brake technology and Overload protection"]
["Main gearbox type ","Super duty twin drive gears driving the main output gear"]
["Flywheel speed (rpm) ","1440"]
["Standard Packer system"]
["Standard Packer system ","Standard"]
["Feeder ","3 packer forks / 9 single tines"]
["Feed assist auger ","Standard"]
["5 bar MaxiSweep™ Pick-up"]
["Width (DIN 11220) (m) ","2.35"]
["Roller windguard ","Standard"]
["Number of double Tines / Tine diameter (mm) ","85 / 5.5"]
["Flotation ","Adjustable spring"]
["Gauge wheels / Castering gauge wheels ","Standard / Optional"]
["Standard tyres / HD tyres ","Standard / Optional"]
["Pick up slipclutch protection ","Standard"]
["CropCutter™ system"]
["CropCutter™ system ","Optional"]
["No. Knives (mm) ","15 (Medium Cut) or 29 (Short Cut)"]
["Knife removal ","Sliding knife drawer"]
["Knife activation, in - out ","Hydraulic"]
["Knife protection ","Individual springs"]
["Feed assist auger ","Standard"]
["Hydraulic feed assist auger with reverse functionality ","Optional"]
["Rotor ","Width 1200 mm «W» tine configuration with paired rotor fingers per knife"]
["Hard faced rotor ","Optional"]
["Rotor protection ","Cut-out clutch"]
["Stuffer"]
["Stuffer ","Fork type with 6 tines"]
["Stuffer protection ","Shearbolt"]
["SmartFill™ II system ","Standard"]
["Plunger"]
["Speed (Strokes/min) ","48"]
["Length of stroke (mm) ","748"]
["Tying system"]
["Type ","Loop Master™ double knot type"]
["Twine type ","100-130m/kg grade"]
["Number of twines ","6"]
["Knotter fan type ","Electric"]
["Number of Knotter fans ","6 Optional"]
["Electronic Bale Length / Knotter engagement system ","Standard"]
["Knotter function alert ","IntelliView™ monitor and Knotter flags"]
["Knotter lubrication ","Grease"]
["Twine ball capacity ","36 XL"]
["Hydraulic foldable twine boxes ","Standard"]
["Needle cleaning kit ","Optional"]
["Bale density system"]
["7 double acting cylinders proportional controlled ","IntelliView™ monitor controlled"]
["Electronic control system"]
["ISOBUS compatible with AEF ISOBUS certification ","Standard"]
["ISOBUS III IntelliCruise™ system ","Optional"]
["IntelliSense™ ","Optional"]
["IntelliView™ IV Plus ","Optional"]
["IntelliView™ IV ","Optional"]
["FieldOps™ ","Optional"]
["Lights"]
["Standard LED work lights ","Front & rear road lights, 2 x rear work lights, LED strip lights on the knotter, pickup and needles"]
["Optional LED Service lights ","Left and right hand side stuffer lights, left and right hand side twine box lights"]
["Axles"]
["Large wheel tandem axle with Auto-Steer system (Tyre size) ","600/50R22.5 or 600/55R26.5"]
["Hydraulic suspension ","Standard"]
["Brakes"]
["Pneumatic / Hydraulic ","Standard / Optional"]
["Maximum travelling speeds"]
["Large wheel tandem axle (Kph) ","60*"]
["Baler dimensions"]
["Length chute closed (mm) ","8936"]
["Width (mm) ","2987"]
["Height folded railing up (mm) ","3440"]
["Height folded railing down (mm) ","3099"]
["Weight (Empty on 600/55R26.5) (kg) ","Standard Packer 14300kg / CropCutter™ 14600kg"]
["Equipment"]
["Standard equipment ","Roller windguard, Automatic greasing system, Standard Bale-Eject™ system, Roller bale chute with hydraulic folding, Foldable railing"]
["Optional equipment ","Comfort pack, Partial bale-Eject™, Comfort Baler Height adjustment, Camera monitoring system, ActiveWeigh™ system,\nRub pad or Starwheel Moisture measuring system, Additional 3 electric driven knotter fans,\nknotter blow off kit, needle cleaner kit, Rear Bumper, Abrasive option rotor"]
["* Pneumatic brake version only"]