{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":70,"n_cols":5,"rows_kept":70,"cut":false,"hidden":false,"merged":[[69,0,69,6]]}
[]
[null,"T3.50F","T3.55F","T3.65F","T3.75F"]
["New Holland-motorer"]
["New Holland-motorer ","Serien S8000","Serien S8000","Serien S8000","Serien S8000"]
["Antal cylindrar / Ventiler ","2025-03-02","2025-03-02","2025-03-02","2025-03-02"]
["Utsläppsnivå ","Tier 3 / Steg 3A","Tier 3 / Steg 3A","Tier 3 / Steg 3A","Tier 3 / Steg 3A"]
["Cylindervolym (cm³) ","2 930","2 930","2 930","2 930"]
["Luftintag ","TCA","TCA","TCA","TCA"]
["Laddluftkylare ","Standard","Standard","Standard","Standard"]
["Godkänd biodieselblandning ","B100","B100","B100","B100"]
["Nominell motoreffekt ISO TR14396 - ECE R120 (kW/hk) ","36,8/50","40,4/55","47,8/65","53/72"]
["Nominellt motorvarv (varv/min) ","2 300","2 300","2 300","2 300"]
["Max. vridmoment - ISO TR14396 (Nm vid varv/min) ","201 vid 1 400","220 vid 1 400","261 vid 1 400","295 vid 1 400"]
["Ökning av vridmoment ","29,7 %","29,4 %","34,5 %","34,1 %"]
["Horisontellt avgasrör ","Standard","Standard","Standard","Standard"]
["EGR-system för intern avgasåterföring ","Standard","Standard","Standard","Standard"]
["Kylning ","Vätska","Vätska","Vätska","Vätska"]
["Optimal bränsleförbrukning (g/kWh) ",237,238,238,235]
["Standardvolym på dieseltanken (liter) ",50,50,50,50]
["Växellåda"]
["Bakre elektrohydraulisk differentialspärr ","Standard","Standard","Standard","Standard"]
["Oljeisolerat bromssystem ","Standard","Standard","Standard","Standard"]
["12x12 30 km/h- Mek fram-back"]
["12x12 30 km/h- Mek fram-back ","Standard","Standard","Standard","Standard"]
["Min. körhastighet (utan krypväxel) (km/h) ","0,73","0,73","0,73","0,73"]
["20x20 (12x12 version med krypväxel) 30 km/h-Mek fram-back"]
["20x20 (12x12 version med krypväxel) 30 km/h-Mek fram-back ","Tillval","Tillval","Tillval","Tillval"]
["Min. körhastighet (med krypväxel) (km/h) ","0,10","0,10","0,10","0,10"]
["12x12 40 km/h - Mek fram-back"]
["12x12 40 km/h - Mek fram-back ","Tillval","Tillval","Tillval","Tillval"]
["Min. körhastighet (utan krypväxel) (km/h) ","0,89","0,89","0,89","0,89"]
["20x20 (12x12 version med krypväxel) 40 km/h-Mek fram-back"]
["20x20 (12x12 version med krypväxel) 40 km/h-Mek fram-back ","Tillval","Tillval","Tillval","Tillval"]
["Min. körhastighet (med krypväxel) (km/h) ","0,12","0,12","0,12","0,12"]
["Framaxel"]
["4WD framaxel ","Standard","Standard","Standard","Standard"]
["Vändradie 4WD framaxel (mm) ","3 400","3 400","3 400","3 400"]
["Begränsad slirning, differentialspärr ","Standard","Standard","Standard","Standard"]
["Fristående styrpump (32 l/m) ","Standard","Standard","Standard","Standard"]
["Axelpendling (°) ",11,11,11,11]
["Hydraulsystem"]
["Standard pumpflöde (l/m) ",52,52,52,52]
["Mekaniskt dragkraftsreglage (MDC) ","Standard","Standard","Standard","Standard"]
["Lift-O-Matic™-system ","Standard","Standard","Standard","Standard"]
["Lyftens maximala kapacitet vid kopplingspunkterna med horisontella armar (kg) ","2 277","2 277","2 277","2 277"]
["Trepunktslyft kategori I och II med snabbkopplingar ","Standard","Standard","Standard","Standard"]
["Max. antal bakre tipputtagsventiler ","3 (6 kopplingar)","3 (6 kopplingar)","3 (6 kopplingar)","3 (6 kopplingar)"]
["Flödeskontroll ","Tillval","Tillval","Tillval","Tillval"]
["Kraftuttag"]
["Servostyrd inkoppling ","Standard","Standard","Standard","Standard"]
["Drivhjulsberoende kraftuttag ","Tillval","Tillval","Tillval","Tillval"]
["540 / 540E varv/min ","Standard","Standard","Standard","Standard"]
["Förarmiljö"]
["Plattform med fjädring och nedfällbart mittmonterat ROPS-skydd ","Standard","Standard","Standard","Standard"]
["Vikter*"]
["Total vikt (kg) ","2 200","2 200","2 200","2 200"]
["Dimensioner**"]
["Bakdäck min. ","320/70R20","320/70R20","320/70R20","320/70R20"]
["Bakdäck max. ","360/70R24","360/70R24","360/70R24","360/70R24"]
["Framdäck min. ","200/70R16","200/70R16","200/70R16","200/70R16"]
["Framdäck max. ","280/70R16","280/70R16","280/70R16","280/70R16"]
["Framaxelns markfrigång (mm) ",215,215,215,215]
["Total bredd min. (mm) ","1 350","1 350","1 350","1 350"]
["Total bredd max. (mm) ","1 710","1 710","1 710","1 710"]
["Hjulbas (mm) ","1 863","1 863","1 863","1 863"]
["Längd (mm) ","3 438","3 438","3 438","3 438"]
["Rattens höjd (mm) ","1 235","1 235","1 235","1 235"]
["Total höjd (mm) ","2 246","2 246","2 246","2 246"]
["Sätets höjd (mm) ",995,995,995,995]
["            * med 200/70R16 - 320/70R20 däck tyres        \n** med däcken 200/70R16 - 320/70R20 ​"]