{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[21,0,21,6]]}
[]
[null,"740CF Superflex™ skärbord - 20 ft.","740CF Superflex™ skärbord - 25 ft.","740CF Superflex™ skärbord - 30 ft.","740CF Superflex™ skärbord - 35 ft."]
["Teknisk Information"]
["740CF Superflex skärbord (ft) ",20,25,30,35]
["Skärbredd (m) ","2025-06-01","7,62","2025-09-15","10,67"]
["Knivhastighet (skärn./min.) ",650,650,650,650]
["Knivslag (mm / “) ","80 / 3","80 / 3","80 / 3","80 / 3"]
["Vertikal knivflexibilitet (mm / “) ","152 / 6","152 / 6","152 / 6","152 / 6"]
["Reservkniv ","Tillval","Tillval","Tillval","Tillval"]
["Drivning en kniv ","Standard","Standard","Standard","Standard"]
["Drivning två knivar ","–","–","Tillval","Tillval"]
["Inmatningsskruven diameter (mm) ",660,660,660,660]
["Inmatningsskruv med indragbara pinnar i full bredd ","Standard","Standard","Standard","Standard"]
["Skruvens hastighet (v/min) ",147,147,147,147]
["Haspeldiameter (m) ","2025-01-07","2025-01-07","2025-01-07","2025-01-07"]
["Avstånd mellan kniv och inmatningsskruv (mm) ",369,369,369,369]
["Autofloat™ system ","Standard","Standard","Standard","Standard"]
["Medelstor stråskiljare ","Standard","Standard","Standard","Standard"]
["Lång stråskiljare ","Tillval","Tillval","Tillval","Tillval"]
["Stubbskärmar ","Tillval","Tillval","Tillval","Tillval"]
["Vikt (kg/lbs) ","1830/4034","2206/4863","2560/5644*","3132/6905*"]
["* Drivning med en kniv"]