{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":96,"n_cols":5,"rows_kept":96,"cut":false,"hidden":false,"merged":[[95,0,95,6]]}
[]
[null,"T6020 Plus","T6050 Plus","T6070 Plus","T6070 Elite"]
["New Holland Engine*"]
["New Holland Engine* ","FPT","FPT","FPT","FPT"]
["No. of cylinders / capacity / Valves / Emissions Level ","4 / 4485 / 2 / Tier III","6 / 6728 / 2 / Tier III","6 / 6728 / 2 / Tier III","6 / 6728 / 4 / Tier III"]
["Aspiration ","Turbocharged","Turbocharged","Turbocharged","Turbocharged"]
["Intercooler ","Standard","Standard","Standard","Standard"]
["Fuel system - High pressure common rail ","–","–","–","Standard"]
["Approved Biodiesel Blend ","B100**","B100**","B100**","B100**"]
["Rated Engine Power - ISO TR14396 - ECE R120 [kW/hp] ","82 / 112","93 / 127","104 / 141","104 / 141"]
["Rated power with EPM - ISO 14396 - ECE R120 [kW/hp] ","–","–","–","123 / 167"]
["Max. power - ISO 14396 - ECE R120 [kW/hp] ","82 / 112","93 / 127","104 / 141","112 / 152"]
["Max. power with EPM - ISO 14396 - ECE R120 [kW/hp] ","–","–","–","131 / 178"]
["Rated Engine Speed (rpm) ",2200,2200,2200,2200]
["Max. Torque ISO TR14396 - ECE R120 at 1400rpm (Nm) ",510,555,625,613]
["Max. torque with EPM - ISO 14396 - ECE R120 (Nm) ","–","–","–",678]
["Torque rise standard / with EPM (%) ","43 / –","38 / –","39 / –","35 / 27"]
["Engine Power Management (EPM) ","–","–","–","Standard"]
["Engine Speed Management (ESM) ","–","–","–","Standard"]
["Exhaust aspirated pre cleaner ","Standard","Standard","Standard","Standard"]
["Fuel tank capacity (l) ",176,250,250,250]
["Service Interval (hrs) ",600,600,600,600]
["A pillar mounted exhaust ","Standard","Standard","Standard","Standard"]
["Alternator (Amps) ",120,120,120,150]
["Transmission"]
["Electro Command™ transmission (40kph) ","Standard","Standard","Standard","Standard"]
["Power Shuttle ","Standard","Standard","Standard","Standard"]
["Number of gears / with Creeper (F x R) ","16 x 16 / 32 x 32","16 x 16 / 32 x 32","16 x 16 / 32 x 32","16 x 16 / 32 x 32"]
["Minimum speed / Minimum speed with Creeper (kph) ","2.23 / 0.19","2.23 / 0.19","2.23 / 0.19","2.23 / 0.19"]
["IntelliShift™ System ","Standard","Standard","Standard","Standard"]
["Active Electro Command™ auto transmission functions ","Standard","Standard","Standard","Standard"]
["Active Electro Command™ transmission (50kph) ","Optional","Optional","Optional","Optional"]
["Rear Axle - Bar Type ","-","-","-","-"]
["Rear Axle - Flange Type ","Standard","Standard","Standard","Standard"]
["Front Axle"]
["4WD Front Axle ","Standard","Standard","Standard","Standard"]
["SuperSteer™ front axle ","-","Optional","-","-"]
["Terraglide™ front axle suspension ","Optional","Optional","Optional","Optional"]
["Steering angle 4WD / Terraglide™ front axle ","55 / 55","55 / 65 / 55","55 / 55","55 / 55"]
["Terralock™ auto 4WD and diff lock functions ","Standard","Standard","Standard","Standard"]
["Hydraulically locked front differential ","Standard","Standard","Standard","Standard"]
["Dynamic Front Fenders ","Optional","Optional","Optional","Optional"]
["Turning radius with 4WD / Terraglide™ suspended front axle (mm) ",4040,4355,4355,4355]
["Turning radius with SuperSteer™ front axle (mm) ","-","-","-","-"]
["Hydraulic system"]
["CCLS Closed Centre Load Sensing ","Standard","Standard","Standard","Standard"]
["Main pump fl ow / Pump pressure (Lpm / Bar) ","113 / 210","113 / 210","113 / 210","113 / 210"]
["Steering pump fl ow (Lpm) ",47,47,47,47]
["Electronic Draft Control (EDC) ","Standard","Standard","Standard","Standard"]
["Dynamic Ride Control ","Standard","Standard","Standard","Standard"]
["Remote valves"]
["Deluxe load sensing with fl ow control ","Standard","Standard","Standard","Standard"]
["Std / Max. no. rear valves ","2025-02-04","2025-02-04","2025-02-04","2025-02-04"]
["Linkage - Rear"]
["Max. lift capacity at ball ends (kg) ",7864,7864,7864,7864]
["Swinging Drawbar ","Standard","Standard","Standard","Standard"]
["PTO"]
["540 / 540E / 1000 ","Standard","Standard","Standard","Standard"]
["Electro Hydraulic PTO engagement ","Standard","Standard","Standard","Standard"]
["Auto PTO management ","Standard","Standard","Standard","Standard"]
["Cab"]
["360° Horizon™ cab with FOPS - OECD Code 10 Level 1 ","Standard","Standard","Standard","Standard"]
["Horizon cab category level 2 - EN 15695 ","Standard","Standard","Standard","Standard"]
["High visibility roof hatch ","Standard","Standard","Standard","Standard"]
["Deluxe air suspension seat with seat belt ","Standard","Standard","Standard","–"]
["Instructors seat with seat belt ","Standard","–","–","Standard"]
["Air conditioning ","Standard","Standard","Standard","Standard"]
["Air Recirculation Filters ","Standard","Standard","Standard","Standard"]
["Telescopic Shatterproof Mirrors ","Standard","Standard","Standard","Standard"]
["Comfort Ride™ cab suspension ","Standard","Standard","Standard","Standard"]
["Headland Turn Sequencing ","–","–","–","Standard"]
["Fender mounted external PTO & Linkage controls ","Standard","Standard","Standard","Standard"]
["Performance Monitor with enhanced key pad and ISO 11786 connector ","Standard","Standard","Standard","Standard"]
["Cab monitor mounting bracket ","Standard","Standard","Standard","Standard"]
["Optimum Cab Noise level - 77/311EEC (dB(A)) ",70,73,73,71]
["Optimum Seat Vibration level - EN 1032 (m/s) ",1.05,1.05,1.06,1.06]
["Factory Fit Rotating Beacon ","Standard","Standard","Standard","Standard"]
["Cab glass area (m²) ",5.87,5.87,5.87,5.87]
["A pillar mounted exhaust ","Standard","Standard","Standard","Standard"]
["Dimensions on Standard tyres"]
["Overall length inc. rear linkage (all axle types) (mm) ",4145,4385,4385,4385]
["Minimum width (mm) ",2280,2280,2280,2280]
["Height at centre of rear axle to top of Comfort Ride™ suspension cab (mm) ",2165,2165,2165,2165]
["Overall height of Comfort Ride™ suspension cab (mm) ",2965,2965,2965,2965]
["Wheelbase Standard 4WD axle(mm) ",2387,2627,"-",2627]
["Wheelbase SuperSteer 4WD axle (mm) ","-","-",2775,"-"]
["Wheelbase Terraglide™ suspended axle (mm) ",2439,2679,2679,2679]
["Wheelbase Track width (min. / max - tyre size dependent) (mm) ","1325 - 2285","1325 - 2285","1325 - 2285","1325 - 2285"]
["Wheelbase Ground Clearance - Under Drawbar (min / max) (mm) ","260 / 480","260 / 480","260 / 480","260 / 480"]
["Wheelbase Ground Clearance - Front Axle (min / max) (mm) ","320 / 520","320 / 520","320 / 520","320 / 520"]
["Weights"]
["Minimum unballasted / shipping weights 4WD front axle (kg) ",4740,4910,4920,4920]
["Max. permissible weight (kg) ",9000,9000,9000,9000]
["Standard tyres - Front ","420/70R28","420/70R28","420/70R28","420/70R28"]
["Standard tyres - Rear ","520/70R38","520/70R38","520/70R38","520/70R38"]
["* Developed by FPT Industrial - Fiat Powertrain Technologies\n* Shipping weight will vary depending on independent vehicle specifications"]