{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":59,"n_cols":5,"rows_kept":59,"cut":false,"hidden":false,"merged":[[58,0,58,6]]}
[]
[null,"TT4.55","TT4.65","TT4.75","TT4.90"]
["Engine"]
["No. Cylinders / Aspiration / valves / emission level ","3 / T / 2 / Tier III","3 / TI / 2 / Tier III","3 / TI / 2 / Tier III","4 / TI / 2 / Tier III"]
["Approved Biodiesel Blend ","B100","B100","B100","B100"]
["Capacity (Litres) ","2.9","2.9","2.9","3.9"]
["Rated Power ISO TR14396-ECE R120 (kW/hp) @ rated speed ","41 / 55 @ 2300","48 / 65 @ 2300","55 / 75 @ 2300","66 / 88 @ 2300"]
["PTO Power at Rated Speed (kW/hp) ","36.6 / 49","42.5 / 57","48.5 / 66.0","55.2 / 74.0"]
["Maximum Torque (Nm) ","220","270","300","340 @ 1400"]
["Torque Rise (%) ","30","30","30","25"]
["Fuel Capacity (Litres) Main + Auxillary (not applicable on TT4.90) ","60 + 40","60 + 40","60 + 40","90"]
["Transmission"]
["Synchro - Mechanical Forward / Reverse shuttle (Dash mounted) ","Standard","Standard","Standard","N/A"]
["Hydraulic Power Shuttle (Dash mounted) ","Optional","Optional","Optional","Standard"]
["12 x 12 Mechanical Synchromesh transmission ","Standard","Standard","Standard","Standard"]
["Minimum speed / Maximum road speed (kph)* ","1.56 / 32.05","1.56 / 33.23 1.56","1.56 / 34.4","1.72 / 35.8"]
["20 x 20 Mechanical Powershuttle transmission with creeper ","Optional","Optional","Optional","Optional"]
["Creeper - Minimum speed / Maximum road speed (kph)* ","0.27 / 32.05","0.27 / 32.05","0.27 / 32.05","0.30 / 35.8"]
["Front Axles"]
["4WD front axle ","Standard","Standard","Standard","Standard"]
["2WD front axle ","Optional","Optional","Optional","Optional"]
["Steering angle 4WD (°) ","55","55","55","55"]
["Minimum Turn Radius Less Brakes 4WD (mm) ","6.0","6.0","6.4","5.1"]
["Rear Axle"]
["Planetary reduction final drive ","Standard","Standard","Standard","Standard"]
["Differential lock (Mechanically engaged) ","Standard","Standard","Standard","Standard"]
["Oil immersed multidisc braking system ","Standard","Standard","Standard","Standard"]
["Hydraulics"]
["Main pump flow / pump pressure (Lpm / Bar) ","54 / 207","54 / 207","54 / 207","60 / 207"]
["Independent steering pump flow / pump pressure (Lpm / Bar) ","28.8 / 210","28.8 / 210","28.8 / 210","33 / 207"]
["Rear Auxiliary Remote Valves (Std / Max number) ","2 / 3","2 / 3","2 / 3","2 / 3"]
["Linkage"]
["Category ","I / II","I / II","I / II","I / II"]
["Lift capacity @ ball ends ","2500","2500","2500","3500"]
["Lift capacity @ 610mm behind ball ends ","1845","1845","1845","2750"]
["Swinging drawbar ","Standard","Standard","Standard","Standard"]
["PTO"]
["Independent rear PTO ","Standard","Standard","Standard","Standard"]
["Rear PTO ","540 / 540E","540 / 540E","540 / 540E","540 / 540E"]
["Rear PTO Engine Speed at 540 rpm ","2217","2217","2217","2217"]
["Rear PTO Engine Speed at 540E rpm ","1715","1715","1715","1715"]
["Operator environment"]
["Mechanical suspension seat with seat belt on inclined plane ","Standard","Standard","Standard","Standard"]
["Suspension Travel (mm) ","90","90","90","90"]
["Flat deck Operator Area ","Standard","Standard","Standard","Standard"]
["Suspended Brake and Clutch pedals ","Standard","Standard","Standard","Standard"]
["Canopy ","Standard","Standard","Standard","Standard"]
["Two post Foldable ROPS platform ","Standard","Standard","Standard","Standard"]
["Dimensions"]
["Wheelbase 2WD / 4WD (mm) ","2079 / 2010","2079 / 2010","2200 / 2145","2283 / 2258"]
["Overall length with front weights 2WD / 4WD (mm) ","3875","3875","3875","4059"]
["Overall Width 2WD/ 4WD (mm) ","1965","1965","2041","2041"]
["Height to top of ROPS 2WD / 4WD (mm) ","2538","2566","2589","2589"]
["Height to top of Exhaust 2WD / 4WD (mm) ","2435","2464","2487","2487"]
["Height to top of Steering wheel 2WD / 4WD (mm) ","1754","1782","1810","1814"]
["Ground clearance under front axle 2WD / 4WD (mm) ","504","504 ","504","504 / 416"]
["Shipping Weight ROPS 2WD / 4WD (kg) ","2286 / 2640","2400 / 2795","2514 / 2935","2825 / 3085"]
["Maximum ballasted weight 2WD / 4WD (kg) ","2690 / 2755","3080 / 3145","3080 / 3145","3860 / 3990"]
["    * Speed with Standard tyres"]