{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":140,"n_cols":4,"rows_kept":140,"cut":false,"hidden":false,"merged":[[139,0,139,5]]}
[]
[null," T7.190 "," T7.210 "," T7.225 Auto Command™"]
["New Holland engine*"]
["New Holland engine* ","Nef","Nef","Nef"]
["No. of cylinders / Aspiration / Valves ","6 / T / 4","6 / T / 4","6 / T / 4"]
["Compliant with engine emissions regulations ","Stage V","Stage V","Stage V"]
["ECOBlue™ HI-eSCR system (Selective Catalytic Reduction) ","Standard","Standard","Standard"]
["Fuel system - High pressure Common Rail ","Standard","Standard","Standard"]
["Approved biodiesel blend** ","B7","B7","B7"]
["Capacity (cm³) ","6728","6728","6728"]
["Bore and Stroke (mm) ","104x132","104x132","104x132"]
["Max. EPM horsepower - ISO TR14396 - ECE R120 [kW/hp(CV)] ","140 / 190","154 / 210","165 / 225"]
["Max. horsepower - ISO TR14396 - ECE R120 [kW/hp(CV)] ","121 / 165","132 / 180","147 / 200"]
["Rated EPM horsepower - ISO TR14396 - ECE R120 [kW/hp(CV)] ","129 / 175","140 / 190","151 / 205"]
["Rated horsepower - ISO TR14396 - ECE R120 [kW/hp(CV)] ","110 / 150","121 / 165","132 / 180"]
["Rated engine speed (rpm) ","2200","2200","2200"]
["Max. EPM torque - ISO TR14396 (Nm) ","805@1500rpm","875@1500rpm","940@1500rpm"]
["Max. torque ISO TR14396 (Nm) ","700@1500rpm","770@1500rpm","840@1500rpm"]
["Torque rise Standard / EPM (%) ","46 / 44","46 / 44","46 / 44"]
["Reversible fan ","Optional","Optional","Optional"]
["Exhaust brake ","Optional","Optional","Optional"]
["Diesel tank capacity Standard / Optional (Litres) ","330","330","330"]
["AdBlue tank capacity (Litres) ","48","48","48"]
["Service interval (hours) ","750","750","750"]
["Range Command™ transmission"]
["IntelliShift™ system ","Standard","Standard","–"]
["Powershuttle lever with aggressiveness setting switch ","Standard","Standard","–"]
["Auto transmission functions ","Standard","Standard","–"]
["Range Command™ Semi-powershift (40kph) ","Optional","–","–"]
["Number of gears / with Creeper (FxR) ","18x6 / 28x12","–","–"]
["Min. speed / Min. speed with Creeper (kph) ","2.2 / 0.37","–","–"]
["Range Command™ Semi-powershift (40kph ECO or 50kph) ","Optional","Optional","–"]
["Low mount window wiper ","–","–","–"]
["Power Command™ transmission"]
["IntelliShift™ system ","Standard","Standard","–"]
["Powershuttle lever with aggressiveness setting switch ","Standard","Standard","–"]
["Auto transmission functions ","Standard","Standard","–"]
["Power Command™ Full Powershift (40kph) ","Optional","Optional","–"]
["Number of gears / with Creeper (FxR) ","18x6 / 28x12","18x6 / 28x12","–"]
["Min. speed / Min. speed with Creeper (kph) ","1.8 / 0.29","1.8 / 0.29","–"]
["Power Command™ Full Powershift (40kph ECO or 50kph) ","Optional","Optional","–"]
["Low mount window wiper ","Standard","Standard","–"]
["Auto Command™ Continuously Variable Transmission"]
["Powershuttle lever with aggressiveness setting switch ","Standard","Standard","Standard"]
["Active StopStart function ","Standard","Standard","Standard"]
["Force base propulsion control ","Standard","Standard","Standard"]
["Auto Command™ Continuously Variable Transmission (40kph ECO) ","Standard","Standard","Standard"]
["Min. speed / Max. speed (kph) ","0.02 / 40@1550rpm","0.02 / 40@1550rpm","0.02 / 40@1550rpm"]
["Auto Command™ Continuously Variable Transmission (50kph ECO) ","Optional","Optional","Optional"]
["Low mount window wiper ","Standard","Standard","Standard"]
["Electrical"]
["12 volt alternator Standard / Optional (Amps) ","120 / 150 / 200","120 / 150 / 200","150 / 200"]
["Battery capacity (CCA / Ah) ","960 / 132","960 / 132","960 / 132"]
["Axles"]
["4WD front axle ","Standard","Standard","Standard"]
["Terraglide™ front axle suspension ","Optional","Optional","Optional"]
["SuperSteer™ front axle ","Optional","Optional","Optional"]
["Steering angle Standard / Terraglide™ / SuperSteer™ axle (°) ","55 / 55 / 65","55 / 55 / 65","55 / 55 / 65"]
["CustomSteer™ system ","Optional","Optional","Optional"]
["Terralock™ functions ","Standard","Standard","Standard"]
["Dynamic front fenders ","Optional","Optional","Optional"]
["Bar rear axle ","Optional","Optional","Optional"]
["Turning radius with SuperSteer™ front axle (mm) ","4950","4950","4950"]
["Turning radius with Standard / Terraglide™ suspension front axle (mm) ","5450","5450","5450"]
["Hydraulics"]
["Closed Centre Load Sensing (CCLS) ","Standard","Standard","Standard"]
["Range & Power Command - Main pump flow Standard / MegaFlow™ option (Lpm) ","113","113","–"]
["Auto Command - Main pump flow Standard / MegaFlow™ option (Lpm) ","140 / 160","140 / 160","140 / 160"]
["Electronic Draft Control (EDC) ","Standard","Standard","Standard"]
["Max. no. rear valves ","4","4","5"]
["Max. no. Deluxe rear valves ","4","4","–"]
["Max. no. electro hydraulic rear valves ","5","5","5"]
["Advanced Joystick control (Forward / Reverse + Gear Change) ","Optional","Optional","Optional"]
["Max. no. mid mount valves ","3","3","3"]
["Linkage"]
["Max. lift capacity at ball ends (kg) ","8257","8257","8257"]
["Max. lift capacity through the range (610mm behind ball ends) (kg) ","6616","6616","6616"]
["Front linkage lift capacity at ball ends (through the range) (kg) ","3568","3568","3568"]
["Front loader ready ","Optional","Optional","Optional"]
["Seat mounted integrated loader joystick ","Standard","Standard","Standard"]
["Brakes"]
["Range and Power Command electronic park brake ","Optional","Optional","Optional"]
["Auto Command electronic park brake ","Standard","Standard","Standard"]
["Hydraulic trailer brakes ","Optional","Optional","Optional"]
["Pneumatic trailer braking system ","Optional","Optional","Optional"]
["PTO"]
["Auto Soft Start ","Standard","Standard","Standard"]
["Engine speed at: 540 / 1000 (rpm) ","1969 / 1924","1969 / 1924","1969 / 1924"]
["Engine speed at: 540 / 540E / 1000 (rpm) ","1969 / 1546 / 1893","1969 / 1546 / 1893","1969 / 1546 / 1893"]
["Engine speed at: 540E / 1000 / 1000E (rpm) ","1592 / 1893 / 1621","1592 / 1893 / 1621","1592 / 1893 / 1621"]
["Auto PTO management ","Optional","Optional","Optional"]
["Front PTO (1000rpm) ","Optional","Optional","Optional"]
["Cab"]
["Four pillar 360° Horizon™ cab with FOPS - OECD code 10 level 1 ","Standard","Standard","Standard"]
["Horizon™ cab category level - EN 15695 ","2","2","2"]
["High visibility roof hatch - Low roof / High roof ","– / Optional","– / Optional","– / Optional"]
["Opening RHS door ","Optional","Optional","Optional"]
["Heated front and rear windscreen ","Optional","Optional","Optional"]
["8 Halogen lighting pack - Low roof / Hi roof ","–","–","–"]
["8 LED lighting pack ","Standard","Standard","Standard"]
["12 LED lighting pack ","Optional","Optional","Optional"]
["16 LED lighting pack ","Optional","Optional","Optional"]
["20 LED lighting pack ","Optional","Optional","Optional"]
["Comfort seat with seat belt ","Optional","Optional","Optional"]
["Dynamic Comfort™ seat with seat belt ","Optional","Optional","Optional"]
["Auto Comfort™ Active Climate Control, leather seat with seat belt ","Optional","Optional","Optional"]
["Instructors seat with seat belt ","Optional","Optional","Optional"]
["Luxury Pack (Leather Steering wheel and carpet) ","Optional","Optional","Optional"]
["Blue Power Package: Metallic Blue and Silver paint, branded seats and carpet ","Optional","Optional","Optional"]
["Air conditioning ","Standard","Standard","Standard"]
["Automatic climate control ","Optional","Optional","Optional"]
["MP3 Bluetooth radio (hands free phone calls) ","Optional","Optional","Optional"]
["Telescopic shatterproof mirrors ","Standard","Standard","Standard"]
["Wide Angle Telescopic Shatterproof Mirrors ","Optional","Optional","Optional"]
["Comfort Ride™ cab suspension ","Optional","Optional","Optional"]
["Fender mounted external PTO & linkage controls ","Optional","Optional","Optional"]
["Fender mounted external remote valve control ","Optional","Optional","Optional"]
["Range and Power Command optimum cab noise level - 77 / 311EEC [dB(A)] ","70","70","70"]
["Auto Command optimum cab noise level - 77 / 311EEC [dB(A)] ","69","69","69"]
["Factory fit rotating beacons (1 / 2) ","Optional","Optional","Optional"]
["FieldOps™"]
["Classic armrest ","Optional","Optional","–"]
["SideWinder™ II armrest ","Optional","Optional","Standard"]
["CommandGrip™ handle ","Optional","Optional","Standard"]
["Performance Monitor with enhanced key pad and ISO 11786 connector ","Optional","Optional","Optional"]
["Auto Command™ IntelliView™ IV Plus colour monitor with ISO 11783 connector ","Standard","Standard","Standard"]
["Dual IntelliView™ IV Plus colour monitor with ISO 11783 connector ","Optional","Optional","Optional"]
["Camera Connection ","Optional","Optional","Optional"]
["Cab monitor mounting bracket ","Optional","Optional","Optional"]
["IntelliSteer® guidance ready ","Optional","Optional","Optional"]
["Headland Turn Sequencing (HTS) ","Standard","Standard","Standard"]
["IntelliTurn™ with Headland Turn Sequencing (HTS) system ","Optional","Optional","Optional"]
["ISOBUS Class II (External and in cab connection) ","Optional","Optional","Optional"]
["ISOBUS Class III (External and in cab connection) ","Optional","Optional","Optional"]
["FieldOps™ (Connectivity Included) ","Optional","Optional","Optional"]
["Weights (Range & Power Command / Auto Command) Minimum unballasted / shipping weights"]
["Standard front axle (kg) ","6400 / 6450","6400 / 6450","6400 / 6450"]
["Terraglide™ suspended front axle (kg) ","6700 / 6750","6700 / 6750","6700 / 6750"]
["Max. permissible weight at 50kph (Class 4) (kg) ","10500 / 11500","10500 / 11500","11500"]
["            * Developed by FPT Industrial       \n** Biodiesel blend must fully comply with the latest fuel specification EN14214:2009 and operation is in accordance with operator manual guidelines       \n*** Only 40kph ECO @ 1890rpm on 580/70R42 tyres       \n**** 20 LED lights: 16 LED cab lights + 4 LED hood lights       \n***** Hi roof only"]