{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":52,"n_cols":4,"rows_kept":52,"cut":false,"hidden":false,"merged":[[51,0,51,5]]}
[]
[null,"TD80","TD90","TD95"]
["Engine"]
["Engine ","New Holland S8000","New Holland S8000","New Holland S8000"]
["No. of cylinders / Aspiration / Emission level ","4 / Naturally / Tier 2","4 / Turbocharged / Tier 2","4 / Turbocharged / Tier 2"]
["Capacity (cm³) ",3908,3908,3908]
["Bore x stroke (mm) ","104 x 115","104 x 115","104 x 115"]
["Rated engine power ISO TR14396 @ 2000/25/EC [kW/hp(CV)] ","58.8 / 80","65.4 / 89","72.1 / 98"]
["Rated engine speed (rpm) ",2500,2500,2500]
["Max. torque at 1500rpm (Nm) ",298,352,370]
["Torque rise (%) ",25,42,31]
["Fuel tank capacity (l) ",77,77,77]
["Transmission"]
["Synchro Command™ transmission - 30kph - Number of gears (F - R) ","12 x 4","–","–"]
["Speed range (kph) ","2030-01-07","–","2030-01-08"]
["Synchro Shuttle™ transmission - 30kph - Number of gears (F - R) ","12 x 12","12 x 12","12 x 12"]
["Number of gears with creeper (F - R) ","20 x 12","20 x 12","20 x 12"]
["Speed range with creeper (kph) ","0.25-30","0.25-30","0.25-30"]
["Hydraulics"]
["Flexion Bar lower link draft sensing ","Standard","Standard","Standard"]
["Rear linkage category ","II","II","II"]
["Mechanical lift with Lift-O-Matic™ ","Standard","Standard","Standard"]
["Position, draft, mixed and float controls ","Standard","Standard","Standard"]
["Hydraulic pump flow – standard (lpm) ",40.1,40.1,40.1]
["Hydraulic pump flow – MegaFlow™ (l/min) ",51.7,51.7,51.7]
["Steering pump flow (lpm) ",26.5,26.5,26.5]
["Max. number of remote valves ",3,3,3]
["Linkage"]
["Maximum lift capacity at ball ends with arms horizontal (kg) ",3565,3565,3565]
["Continous lift capacity through the range (610mm behind bar ends) (kg) ",2700,2700,2700]
["PTO"]
["540 rpm (rpm) ",2200,2200,2200]
["540 Economy rpm (rpm) ",1715,1715,1715]
["1000 rpm (rpm) ",2381,2381,2381]
["PTO activation ","Mechanical","Mechanical","Mechanical"]
["Turn angle 2WD / 4WD (°) ","55 / 50","55 / 50","– / 50"]
["Min. turn radius 2WD / 4WD (mm) ","3900 / 5100","3900 / 5100","– / 5200"]
["Dimensions"]
["Overall length 2WD / 4WD (mm) ","3921 / 3865","3921 / 3865","– / 3948"]
["Minimum width (mm) ",1808,1808,1808]
["Height at centre of rear axle to top of ROPS (mm) ",1788,1788,1788]
["Total height with ROPS (mm) ",2488,2513,2558]
["Wheelbase 2WD / 4WD ","2248 / 2192","2248 / 2192","– / 2275"]
["Track width - Front 2WD (mm) ","1405-1905","1405-1905","1485-1985"]
["Track width - Front 4WD (mm) ","1560-2000","1560-2000","1560-2000"]
["Track width - Rear min. / Max. (all axle types) (mm) ","1400-2000","1400-2000","1400-2000"]
["Ground clearance, front axle lowest point 2WD / 4WD (mm) ","525 / 390","555 / 415","– / 465"]
["Weights"]
["Unballasted weight 2WD / 4WD (kg) ","2650 / 3080","2650 / 3080","– / 3250"]
["Max. permissible weight on the front axle 2WD / 4WD (kg) ","2500 / 2800","2500 / 2900","– / 3000"]
["Max. permissible weight on the rear axle (kg) ",4150,4150,4250]
["             Standard         Optional – Not available"]