{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":51,"n_cols":2,"rows_kept":51,"cut":false,"hidden":false,"merged":[[50,0,50,3]]}
[]
[null,"TD95D HC "]
["Engine*"]
["No. of cylinders / aspiration / emission level ","4 / turbocharged / Tier 2"]
["Capacity (cm³) ","3908"]
["Rated engine power ISO TR14396 – 2000/25/EC [kW/hp] ","69 / 94"]
["PTO power [kW/hp] ","60 / 81"]
["Rated engine speed (rpm) ","2500"]
["Max. torque at 1500rpm (Nm) ","337"]
["Torque rise (%) ","33"]
["Fuel tank capacity (l) ","115"]
["Synchro Shuttle™ transmission - 30kph"]
["Number of gears with creeper (F - R) ","20x12"]
["Speed range with creeper (kph) ","0.25-30"]
["Axles"]
["4WD front axle ","Standard"]
["Turn angle (°) ","50"]
["Min. turn radius (mm) ","4200"]
["Tyres"]
["Tyre size (Front / Rear) Option 1 ","13.6R38"]
["Tyre size (Front / Rear) Option 2 ","320/80R42"]
["Hydraulics"]
["Main Pump flow - MegaFlow™ (lpm) ","52"]
["Steering pump flow (lpm) ","26.5"]
["Remote valves"]
["Std / Max number ","3 / 4"]
["Linkage"]
["Flexion Bar™ lower link draft sensing ","Standard"]
["Rear linkage category ","II"]
["Mechanical lift with Position, draft, mixed and float controls & Lift-O-Matic™ ","Standard"]
["Maximum lift capacity at ball ends with arms horizontal (kg) ","3565"]
["Continuous lift capacity through the range (610mm behind ball ends) (kg) ","2700"]
["PTO"]
["Engine speed at: 540 / 1000 (rpm) ","2200 / 2380"]
["Cab"]
["Comfort driver seat ","Standard"]
["Air re-circulation filters ","Standard"]
["Dimensions**"]
["Overall length (mm) ","4150"]
["Minimum width (mm) ","1870"]
["Height at centre of rear axle to top of Cab (mm) ","2160"]
["Total height Cab (mm) ","2990"]
["Wheelbase Cab (mm) ","2149"]
["Track width front / rear ","1540-2054 / 1504-2021"]
["Ground clearance (mm) ","635"]
["Weights**"]
["Minimum weight Cab 4WD (kg) ","4,000"]
["Minimum weight ROPS 4WD (kg) ","3,500"]
["Max. permissible weight on the front axle 4WD (kg) ","4,000"]
["Max. permissible weight on the rear axle (kg) ","4,250"]
["    * New Holland Engine developed by FPT        \n** National restrictions apply"]