{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[[19,0,19,10]]}
[]
[null,"New Holland DuraDisc™ 240","New Holland DuraDisc™ 280","New Holland DiscCutter™ 280","New Holland DiscCutter™ 280P","New Holland DiscCutter™ 320","New Holland DiscCutter™ 320P","New Holland DiscCutter™ 360","New Holland DiscCutter™ 390"]
["Specifications"]
["Mounting type ","Rear mounted","Rear mounted","Rear mounted","Rear mounted","Rear mounted","Rear mounted","Rear mounted","Rear mounted"]
["Working width (m) ","2.37","2,77","2.77","2.77","3.11","3.11","3.52","3.86"]
["Conditioner type ","–","–","–","PE-fingers","–","PE-fingers","–","–"]
["Flotation type ","Mechanical","Mechanical","Vari-Float","Vari-Float","Vari-Float","Vari-Float","Vari-Float","Vari-Float"]
["Swath width (m) ","1.8","2.2","2.2","1.2 - 2.5","2.6","1.2 - 2.8","2.95","3.3"]
["TopDry™ wide spreading (m) ","–","–","–","2.5","–","2.8","–","–"]
["Blade type ","Profile blade ","Profile blade ","Twisted blades","Twisted blades","Twisted blades","Twisted blades","Twisted blades","Twisted blades"]
["Number of discs/blades ","6/12","7/14","7/14","7/14","8/16","8/16","9/18","10/20"]
["Easy Lift ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Minimum PTO Power [kW/hp(CV)] ","35/48","40/54","40/54","54/73","50/68","66/90","60/82","70/95"]
["Hydraulic remote required ","1 SA","1 SA","2 SA + 1DA","2 SA + 1DA","2 SA + 1DA","2 SA + 1DA","2 SA + 1DA","2 SA + 1DA"]
["Power take-off ","1⅜ - 6 splines","1⅜ - 6 splines","1⅜ - 6 splines","1⅜ - 6 splines","1⅜ - 6 splines","1⅜ - 6 splines","1⅜ - 6 splines","1⅜ - 6 splines"]
["PTO speed (rpm) ","540","540","540/1000","1000","540/1000","1000","1000","1000"]
["Linkage category ","II","II","II","III","III","III","III","III"]
["Transport height (m) ","3.25","3.65","3.65","3.65","3.99","3.99","4.39*","4.73*"]
["Weight (kg) ","495","555","815","1060","860","1140","940","1060"]
["    * Optional horizontal transport position aviabile menaing below 4m ​​​"]