{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
[]
[null,"T4.80F","T4.90F","T4.100F","T4.110F","T4.80V","T4.90V","T4.100V","T4.110V"]
["Power"]
["Engine Horsepower ","74","84","98","106","74","84","98","106"]
["PTO Horsepower ","65","75","86","93","65","75","86","93"]
["Operator’s platform ","Cab or ROPS","Cab or ROPS","Cab or ROPS","Cab or ROPS","Cab or ROPS","Cab or ROPS","Cab or ROPS","Cab or ROPS"]
["Front Axle ","2WD or 4WD","2WD or 4WD","2WD or 4WD","2WD or 4WD","2WD or 4WD","2WD or 4WD","2WD or 4WD","2WD or 4WD"]
["Transmission Offering"]
["Mechanical shuttle ","16x16","16x16","16x16","16x16","16x16","16x16","16x16","16x16"]
["Power shuttle ","16x16 or 32x16","16x16 or 32x16","16x16 or 32x16","16x16 or 32x16","16x16 or 32x16","16x16 or 32x16","16x16 or 32x16","16x16 or 32x16"]
["3-Point Hitch"]
["Lift capacity @ 24 in. (610 mm) (lbs. (kg)) ","4,045 (1835)","4,045 (1835)","4,045 (1835)","4,045 (1835)","4,400 (1996)","4,400 (1996)","4,400 (1996)","4,400 (1996)"]
["Hydraulics"]
["Rear remotes ","2 / 3 / 3 with Diverter","2 / 3 / 3 with Diverter","2 / 3 / 3 with Diverter","2 / 3 / 3 with Diverter","2 / 3 / 3 with Diverter","2 / 3 / 3 with Diverter","2 / 3 / 3 with Diverter","2 / 3 / 3 with Diverter"]
["Steering & service (gpm (Lpm)) ","9.2 (35)","9.2 (35)","9.2 (35)","9.2 (35)","9.2 (35)","9.2 (35)","9.2 (35)","9.2 (35)"]
["Implement pump (gpm (Lpm)) ","16.9 (76.8)","16.9 (76.8)","16.9 (76.8)","16.9 (76.8)","16.9 (76.8)","16.9 (76.8)","16.9 (76.8)","16.9 (76.8)"]
["Optional Implement pump (cab) (gpm (Lpm)) ","21.1 (80)","21.1 (80)","21.1 (80)","21.1 (80)","21.1 (80)","21.1 (80)","21.1 (80)","21.1 (80)"]
["Weights & Dimensions (4WD ROPS)"]
["Weight (lbs. (kg)) ","6,243 (2832)","6,243 (2832)","6,420 (2912)","6,420 (2912)","5,661 (2568)","5,661 (2568)","5,877 (2666)","5,877 (2666)"]
["Overall length (in. (mm)) ","148.8 (3779)","148.8 (3779)","148.8 (3779)","148.8 (3779)","148.8 (3779)","148.8 (3779)","148.8 (3779)","148.8 (3779)"]
["Min. Height to ROPS (in. (mm)) ","89.6 (2275)","89.6 (2275)","89.6 (2275)","89.6 (2275)","91.9 (2336)","91.9 (2336)","91.9 (2336)","91.9 (2336)"]
["Min. Overall width (in. (mm)) ","61.7 (1569)","61.7 (1569)","61.7 (1569)","61.7 (1569)","43.1 (1094)","43.1 (1094)","43.1 (1094)","43.1 (1094)"]
["Min. Height to hood (in. (mm)) ","54.1 (1374)","54.1 (1374)","54.1 (1374)","54.1 (1374)","53.1 (1349)","53.1 (1349)","53.1 (1349)","53.1 (1349)"]
["Weights & Dimensions (4WD Cab)"]
["Weight (lbs. (kg)) ","6,415 (2910)","6,415 (2910)","6,614 (3000)","6,614 (3000)","5,974 (2710)","5,974 (2710)","6,150 (2790)","6,150 (2790)"]
["Overall length (in. (mm)) ","159 (4035)","159 (4035)","159 (4035)","159 (4035)","148.8 (3779)","148.8 (3779)","148.8 (3779)","148.8 (3779)"]
["Min. Height to Cab (in. (mm)) ","95.5 (2425)","95.5 (2425)","95.5 (2425)","95.5 (2425)","94.5 (2400)","94.5 (2400)","94.5 (2400)","94.5 (2400)"]
["Min. Overall width (in. (mm)) ","61.7 (1569)","61.7 (1569)","61.7 (1569)","61.7 (1569)","43.1 (1094)","43.1 (1094)","43.1 (1094)","43.1 (1094)"]
["Min. Height to hood (in. (mm)) ","54.1 (1374)","54.1 (1374)","54.1 (1374)","54.1 (1374)","53.1 (1349)","53.1 (1349)","53.1 (1349)","53.1 (1349)"]
["PTO"]
["Base PTO ","540/540E","540/540E","540/540E","540/540E","540/540E","540/540E","540/540E","540/540E"]
["Optional 1 ","540/1000","540/1000","540/1000","540/1000","540/1000","540/1000","540/1000","540/1000"]