{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":4,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
[]
[null,"5610S","6610S","7610S"]
["Engine"]
["Engine ","FPT, NEF 4 cylinders, 4.5l capacity","S8000","FPT, NEF 4 cylinders, 4.5l capacity"]
["Aspiration ","Naturally aspirated","Turbocharged and Intercooled","Turbocharged and Intercooled"]
["Injection ","Mechanical, BOSCH rotary pump","Direct injection, mechanical injection system","Mechanical, BOSCH rotary pump"]
["Rated power (kW/hp) ","59/80","73 / 98","77/108"]
["Torque @ 1400rpm (Nm) ","320","431","453"]
["Fuel tank (Std. / Opt.) (l) ","80 / –","85 / 135","80 / 130"]
["Transmission"]
["Transmission ","8F 2R Econoshift","8F 2R Econoshift","8F 2R Econoshift"]
["Optional ","16F 4R Dual Power","12F 3R with creeper","16F 4R Dual Power"]
["Clutch ","14“ Cerametallic","14“ Cerametallic","14“ Cerametallic"]
["Lubrication ","Forced with oil cooler","Forced with oil cooler","Forced with oil cooler"]
["4WD engagement / Front diff lock ","Electro-hydraulic / Limited slip","Electro-hydraulic / Limited slip","Electro-hydraulic / Limited slip"]
["PTO ","Independent - Hydraulic engagement","Independent - Hydraulic engagement","Independent - Hydraulic engagement"]
["PTO speed (Std. / Opt.) (rpm) ","540 / –","540 / 540-1000","540 / 540-1000"]
["Hydraulics"]
["Hydraulic system ","Open Centre","Open Centre","Open Centre"]
["Max. hydraulic flow (l/min.) ","51","51v","51"]
["Rear remote (Std. / Opt.) ","1 Open Centre / 2 Close Centre","1 Open Centre / 2 Close Centre","1 Open Centre / 2 Close Centre"]
["Lifting capacity (kg) ","2330","2500","2508"]
["3 Point hitch ","Cat II / Fixed","Cat II / Fixed","Cat II / Fixed"]
["Dedicated pump for steering ","Standard","Standard","Standard"]
["4WD unballasted weight (kg) ","3020","3460","3540"]
["Dimensions and weight"]
["Wheelbase 4WD (mm) ","2330","2384","2330"]
["Front wheel 2WD / 4WD ","7.50x16 / 12.4x24","7.50x16, 10.00x16 / 14.9x24","– / 14.9x24"]
["Rear wheel ","18.4x30","18.4x30, 15.5x38 / 18.4x34","– / 18.4x34"]