{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[]
[null,"760CG Varifeed™ grain header - 16 ft.","760CG Varifeed™ grain header - 18 ft.","760CG Varifeed™ grain header - 20 ft.","760CG Varifeed™ grain header - 22 ft.","760CG Varifeed™ grain header - 25 ft.","760CG Varifeed™ grain header - 28 ft.","760CG Varifeed™ grain header - 30 ft.","760CG Varifeed™ grain header - 35 ft.","760CG Varifeed™ grain header - 41 ft.","Varifeed™ grain header"]
["Specifications"]
["760Cg Varifeed™ grain header (ft) ",16,18,20,22,25,8.5,30,35,41]
["Cutting width (m) ",4.88,5.48,6.1,6.7,7.62,1300,9.15,10.67,12.5]
["Knife speed (cuts/min.) ",1300,1300,1300,1300,1300,"Single (Left hand side)",1300,1300,1300]
["Knife drive ","Single Dual (Left hand side)","Single (Left hand side)","Single (Left hand side)","Single (Left hand side)","Single (Left hand side)",80,"Single (Left hand side)","Single (Left hand side)","Dual (Both sides)"]
["Knife stroke (mm) ",80,80,80,80,80,575,80,80,80]
["Knife travel (mm) ",575,575,575,575,575,"Standard",575,575,575]
["Spare knife and spare bolted knife sections ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Feeding auger with full-width retractable fingers ","Standard","Standard","Standard","Standard","Standard",406,"Standard","Standard","Standard"]
["Feeding auger diameter (mm) ",406,406,406,406,406,1.07,406,406,406]
["Reel diameter (m) ",1.07,1.07,1.07,1.07,1.07,"384-959",1.07,1.07,1.07]
["Distance between knife and in take auger (mm) ","384 - 959","384 - 959","384 - 959","384 - 959","384 - 959","Standard","384-959","384 - 959","384 - 959"]
["Autofloat™ system ","Standard","Standard","Standard","Standard","Standard","Optional","Standard","Standard","Standard"]
["Pivotable adjustable divider ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Short divider ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Fixed short divider ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Optional"]
["Weight (kg/lbs) ","1870/4123","2000/4409","2160/4762","2280/5026","2520/5556","2750/6063","3200/7053","3490/7692","4315/9513"]
["Back sheet extension ","Optional","Optional","Optional","Optional","Optional","Optional","Optional","Standard","Standard"]
["Knife protection & auger stripper plates ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Crop lifter ready ","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard","Standard"]
["Hydraulic side knife ready ","Optional","Optional","Optional","Optional","Standard","Standard","Standard","Standard","Standard"]